<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-AnalogIC-DAC_MCP4725-SOT">
<!-- generated from Sparkfun Eagle Library 'SparkFun-AnalogIC' DAC_MCP4725 SOT -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>The MCP4725 is a low-power, high accuracy, single channel, buffered voltage output 12-bit Digital-to-Analog Convertor (DAC) with non-volatile memory (EEPROM). Its on-board precision output amplifier allows it to achieve rail-to-rail analog output.</description>
<title>MCP4725</title>
<tags>
<tag>SOT</tag>
<tag>DAC_MCP4725</tag>
<tag>SOT23-6</tag>
</tags>
<properties>
<property name="package">SOT23-6</property>
<property name="resolution">12-bit</property>
<property name="family">sparkfun DAC</property>
<property name="chip">MCP4725</property>
<property name="variant">sot</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-analogic_sot23-6_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-analogic_mcp4725_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-analogic_sot23-6_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-analogic_sot23-6_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector3" name="AO" type="male">
<description>AO</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="SCL" type="male">
<description>SCL</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="SDA" type="male">
<description>SDA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="VDD" type="male">
<description>VDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="VOUT" type="male">
<description>VOUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="VSS" type="male">
<description>VSS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>