<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='L3G4200D-Breakout-v10'>
<version>4</version>
<date>2011-11-29</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;strong&gt;Description:&lt;/strong&gt; This is a breakout board for the L3G4200D low-power three-axis angular rate sensor. The L3G4200D has a full scale of &amp;plusmn;250/&amp;plusmn;500/&amp;plusmn;2000 dps and is capable of measuring rates with a user-selectable bandwidth. These work great in gaming and virtual reality input devices, GPS navigation systems and robotics.&lt;/p&gt;


&lt;p&gt;


	&lt;strong&gt;Features:&lt;/strong&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		Three selectable full scales (250/500/2000 dps)&lt;/li&gt;


	&lt;li&gt;


		I2C/SPI digital output interface&lt;/li&gt;


	&lt;li&gt;


		16 bit-rate value data output&lt;/li&gt;


	&lt;li&gt;


		8-bit temperature data output&lt;/li&gt;


	&lt;li&gt;


		Wide supply voltage: 2.4 V to 3.6 V&lt;/li&gt;


	&lt;li&gt;


		Low voltage-compatible IOs (1.8 V)&lt;/li&gt;


	&lt;li&gt;


		Embedded power-down and sleep mode&lt;/li&gt;


	&lt;li&gt;


		Embedded temperature sensor&lt;/li&gt;


	&lt;li&gt;


		High shock survivability&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;strong&gt;Documents:&lt;/strong&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Sensors/Gyros/3-Axis/L3G4200D-Breakout-v10.pdf&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Sensors/Gyros/3-Axis/L3G4200D-Breakout-v10.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Sensors/Gyros/3-Axis/17116.pdf&quot; target=&quot;_blank&quot;&gt;Datasheet&lt;/a&gt; (L3G4200D)&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Sensors/Gyros/3-Axis/L3G4200D_Example.zip&quot; target=&quot;_blank&quot;&gt;Example Code&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://bildr.org/2011/06/l3g4200d-arduino/&quot; target=&quot;_blank&quot;&gt;Bildr Tutorial&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Tri-Axis Gyro Breakout - L3G4200D</title>
<url>http://www.sparkfun.com/products/10612</url>
<tags>
<tag>Gyro</tag>
<tag>Gyroscope</tag>
<tag>Triple Axis</tag>
</tags>
<properties>
<property name='family'>Gyroscope Breakout</property>
<property name='Scales'>Selectable (250, 500, 200 degree/second)</property>
<property name='Comm. Protocol'>Digital</property>
<property name='Operating Voltage'>2.4V - 3.6V</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/L3G4200D-Breakout-v10_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/L3G4200D-Breakout-v10_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/L3G4200D-Breakout-v10_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/L3G4200D-Breakout-v10_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector8' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
<connector id='connector9' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
<connector id='connector10' type='male' name='SCL'>
<description>SCL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad'/><p layer='copper1' svgId='connector10pad'/></pcbView>
</views>
</connector>
<connector id='connector11' type='male' name='SDA'>
<description>SDA</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad'/><p layer='copper1' svgId='connector11pad'/></pcbView>
</views>
</connector>
<connector id='connector12' type='male' name='SDO'>
<description>SDO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='male' name='CS'>
<description>CS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
<connector id='connector14' type='male' name='INT2'>
<description>INT2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector14pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector14pin' terminalId='connector14terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector14pad'/><p layer='copper1' svgId='connector14pad'/></pcbView>
</views>
</connector>
<connector id='connector15' type='male' name='INT1'>
<description>INT1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector15pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector15pin' terminalId='connector15terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector15pad'/><p layer='copper1' svgId='connector15pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
