<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='BMP085 Breakout-v13'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description: &lt;/span&gt;This is a simple breakout board for the BMP085 high-precision, low-power barometric pressure sensor. The BMP085 offers a measuring range of 300 to 1100 hPa with an absolute accuracy of down to 0.03 hPa. It&amp;#39;s based on piezo-resistive technology for EMC robustness, high accuracy and linearity as well as long term stability. This sensor supports a voltage supply between 1.8 and 3.6VDC. It is designed to be connected directly to a micro-controller via the I&amp;sup2;C bus&lt;/p&gt;


&lt;p&gt;


	This breadboard-friendly board breaks out all pins of the BMP085 to a 6-pin 0.1&amp;quot; pitch header. The analog and digital supplies (VDDD and VDDA) of the BMP085 are tied together and broken out to a single pin. We&amp;#39;ve also put two 4.7k pull-up resistors on the I&lt;sup&gt;2&lt;/sup&gt;C lines.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Features:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		Digital two wire (I&lt;sup&gt;2&lt;/sup&gt;C) interface&lt;/li&gt;


	&lt;li&gt;


		Wide barometric pressure range&lt;/li&gt;


	&lt;li&gt;


		Flexible supply voltage range&lt;/li&gt;


	&lt;li&gt;


		Ultra-low power consumption&lt;/li&gt;


	&lt;li&gt;


		Low noise measurement&lt;/li&gt;


	&lt;li&gt;


		Fully calibrated&lt;/li&gt;


	&lt;li&gt;


		Temperature measurement included&lt;/li&gt;


	&lt;li&gt;


		Ultra-flat, small footprint&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Dimensions:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		0.65 x 0.65&amp;quot; (16.5 x 16.5 mm)&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/Sensors/Pressure/BMP085 Breakout-v12.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Components/General/BST-BMP085-DS000-05.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Datasheet&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://dlnmh9ip6v2uc.cloudfront.net/datasheets/Sensors/Weather/BMP085 Breakout-v13.zip&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/tutorials/253&quot;&gt;Quickstart Guide&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/tutorial/Barometric/BMP085_Example_Code.pde&quot; target=&quot;_blank&quot;&gt;Example Arduino Sketch&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/Sensors/Pressure/BMP085 Example Code.zip&quot; target=&quot;_blank&quot;&gt;Example Code&lt;/a&gt; (ATmega328)&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Components/General/BMP085_Flyer_Rev.0.2_March2008.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Product Flyer&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.opencircuits.com/SFE_Footprint_Library_Eagle&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;SFE Eagle Library&lt;/a&gt; has this part!&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://wiring.org.co/learning/libraries/bmp085.html&quot; target=&quot;_blank&quot;&gt;Wiring Example&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://mbed.org/users/tkreyche/notebook/bmp085-pressure-sensor/&quot; target=&quot;_blank&quot;&gt;mbed User Review&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Barometric Pressure Sensor - BMP085 Breakout</title>
<url>http://www.sparkfun.com/products/9694</url>
<tags>
<tag>Barometric</tag>
<tag>Pressure</tag>
<tag>BMP085</tag>
</tags>
<properties>
<property name='family'>Pressure Sensor Breakout</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/BMP085 Breakout-v13_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/BMP085 Breakout-v13_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/BMP085 Breakout-v13_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/BMP085 Breakout-v13_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector5' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector5pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector5pin' terminalId='connector5terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector5pad'/><p layer='copper1' svgId='connector5pad'/></pcbView>
</views>
</connector>
<connector id='connector6' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector6pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector6pad'/><p layer='copper1' svgId='connector6pad'/></pcbView>
</views>
</connector>
<connector id='connector7' type='male' name='EOC'>
<description>EOC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector7pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector7pad'/><p layer='copper1' svgId='connector7pad'/></pcbView>
</views>
</connector>
<connector id='connector8' type='male' name='XCLR'>
<description>XCLR</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
<connector id='connector9' type='male' name='SCL'>
<description>SCL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
<connector id='connector10' type='male' name='SDA'>
<description>SDA</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad'/><p layer='copper1' svgId='connector10pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
