<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-RF-GS406SMD-MATING_SMD_***SPECIAL">
<!-- generated from Sparkfun Eagle Library 'SparkFun-RF' GS406SMD MATING_SMD_***SPECIAL -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>50 Channel GS406 Helical GPS Receiver - SMD Connector.  The Mating SMD SPECIAL is called SPECIAL for a reason. This package was only made in order to make a dummy gs407 PCB with mating connector (used for testing).

sku: GPS-09079</description>
<title>GS406SMD</title>
<tags>
<tag>GS406SMD</tag>
<tag>GS406-MATING_SMD_***SPECIAL</tag>
<tag>MATING_SMD_***SPECIAL</tag>
</tags>
<properties>
<property name="package">gs406-mating_smd_***special</property>
<property name="channels">50</property>
<property name="family">sparkfun GPS module</property>
<property name="chip">GS406</property>
<property name="variant">mating_smd_***special</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-rf_gs406-mating_smd____special_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-rf_gs406smd_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-rf_gs406-mating_smd____special_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/gs406-mating_smd.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector0" name="P1" type="male">
<description>P1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="P10" type="male">
<description>P10</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="P2" type="male">
<description>P2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="P3" type="male">
<description>P3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="P4" type="male">
<description>P4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="P5" type="male">
<description>P5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="P6" type="male">
<description>P6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="P7" type="male">
<description>P7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="P8" type="male">
<description>P8</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="P9" type="male">
<description>P9</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>