<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.b.1486" moduleId="1099ABDE24_ST">
 <version replacedby="20A9BBEE34_ST">1</version>
 <title>Pushbutton</title>
 <label>S</label>
 <date>2008-09-16</date>
 <tags>
  <tag>Pushbutton</tag>
  <tag>button</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">obsolete Switch - 4 pin</property>
  <property name="switching circuit">SPST</property>
  <property name="default state">Normally Open</property>
 <property name="package">THT</property></properties>
 <description>A generic pushbutton.</description>
 <views>
  <iconView>
   <layers image="icon/basic_pbutton.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/basic_pbutton.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
   <schematicView fliphorizontal="true" flipvertical="true">
   <layers image="schematic/pushbutton4lead.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/switch-4lead.svg">
    <layer layerId="copper0"/>
    <layer layerId="keepout"/>
    <layer layerId="soldermask"/>
    <layer layerId="silkscreen"/>
    <layer layerId="outline"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector3" name="Pin 4" type="male">
   <description>pin 4 is always connected with pin 3</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector3pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector3pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector0" name="Pin 1" type="male">
   <description>pin 1 is always connected with pin 2</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="Pin 2" type="male">
   <description>pin 2 is always connected with pin 1</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector2" name="Pin 3" type="male">
   <description>pin 3 is always connected with pin 4</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pad"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
 <buses>
  <bus id="bus0">
   <nodeMember connectorId="connector0"/>
   <nodeMember connectorId="connector1"/>
  </bus>
  <bus id="bus1">
   <nodeMember connectorId="connector2"/>
   <nodeMember connectorId="connector3"/>
  </bus>
 </buses>
</module>