<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-RF-GE863_GPS-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-RF' GE863_GPS  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;GE863 Cellular Module with GPS&lt;/b&gt;
Proto layout and schematic for GE863 cellular module with SiRF III GPS. Spark Fun Electronics SKU : CEL-08246</description>
<title>GE863 Cellular Module with GPS</title>
<tags>
<tag>GE863</tag>
<tag>GE863_GPS</tag>
</tags>
<properties>
<property name="package">ge863</property>
<property name="family">sparkfun GPS</property>
<property name="chip">GE863</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-rf_ge863_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-rf_ge863_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-rf_ge863_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/GE863.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector22" name="ADC_IN1" type="male">
<description>ADC_IN1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector22pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector22pad"/>
</pcbView>
</views>
</connector>
<connector id="connector48" name="ANT" type="male">
<description>ANT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector48pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector48pin" terminalId="connector48terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector48pad"/>
</pcbView>
</views>
</connector>
<connector id="connector29" name="AXE" type="male">
<description>AXE</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector29pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector29pin" terminalId="connector29terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector29pad"/>
</pcbView>
</views>
</connector>
<connector id="connector36" name="C103_TXD" type="male">
<description>C103_TXD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector36pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector36pin" terminalId="connector36terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector36pad"/>
</pcbView>
</views>
</connector>
<connector id="connector37" name="C104_RXD" type="male">
<description>C104_RXD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector37pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector37pin" terminalId="connector37terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector37pad"/>
</pcbView>
</views>
</connector>
<connector id="connector39" name="C105_RTS" type="male">
<description>C105_RTS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector39pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector39pin" terminalId="connector39terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector39pad"/>
</pcbView>
</views>
</connector>
<connector id="connector40" name="C106_CTS" type="male">
<description>C106_CTS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector40pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector40pin" terminalId="connector40terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector40pad"/>
</pcbView>
</views>
</connector>
<connector id="connector42" name="C107_DSR" type="male">
<description>C107_DSR</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector42pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector42pin" terminalId="connector42terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector42pad"/>
</pcbView>
</views>
</connector>
<connector id="connector38" name="C108_DTR" type="male">
<description>C108_DTR</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector38pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector38pin" terminalId="connector38terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector38pad"/>
</pcbView>
</views>
</connector>
<connector id="connector41" name="C109_DCD" type="male">
<description>C109_DCD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector41pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector41pin" terminalId="connector41terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector41pad"/>
</pcbView>
</views>
</connector>
<connector id="connector43" name="C125_RING" type="male">
<description>C125_RING</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector43pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector43pin" terminalId="connector43terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector43pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="CAM_CLK" type="male">
<description>CAM_CLK</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector34" name="CHARGE" type="male">
<description>CHARGE</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector34pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector34pin" terminalId="connector34terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector34pad"/>
</pcbView>
</views>
</connector>
<connector id="connector62" name="DAC_OUT" type="male">
<description>DAC_OUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector62pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector62pin" terminalId="connector62terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector62pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="EAR_HF+" type="male">
<description>EAR_HF+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="EAR_HF-" type="male">
<description>EAR_HF-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="EAR_MT+" type="male">
<description>EAR_MT+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="EAR_MT-" type="male">
<description>EAR_MT-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector16" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector16pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector16pad"/>
</pcbView>
</views>
</connector>
<connector id="connector71" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector71pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector71pin" terminalId="connector71terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector71pad"/>
</pcbView>
</views>
</connector>
<connector id="connector76" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector76pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector76pin" terminalId="connector76terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector76pad"/>
</pcbView>
</views>
</connector>
<connector id="connector78" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector78pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector78pin" terminalId="connector78terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector78pad"/>
</pcbView>
</views>
</connector>
<connector id="connector81" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector81pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector81pin" terminalId="connector81terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector81pad"/>
</pcbView>
</views>
</connector>
<connector id="connector27" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector27pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector27pad"/>
</pcbView>
</views>
</connector>
<connector id="connector35" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector35pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector35pin" terminalId="connector35terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector35pad"/>
</pcbView>
</views>
</connector>
<connector id="connector44" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector44pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector44pin" terminalId="connector44terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector44pad"/>
</pcbView>
</views>
</connector>
<connector id="connector47" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector47pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector47pin" terminalId="connector47terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector47pad"/>
</pcbView>
</views>
</connector>
<connector id="connector49" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector49pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector49pin" terminalId="connector49terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector49pad"/>
</pcbView>
</views>
</connector>
<connector id="connector55" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector55pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector55pin" terminalId="connector55terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector55pad"/>
</pcbView>
</views>
</connector>
<connector id="connector66" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector66pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector66pin" terminalId="connector66terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector66pad"/>
</pcbView>
</views>
</connector>
<connector id="connector68" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector68pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector68pin" terminalId="connector68terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector68pad"/>
</pcbView>
</views>
</connector>
<connector id="connector83" name="GND_GPS" type="male">
<description>GND_GPS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector83pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector83pin" terminalId="connector83terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector83pad"/>
</pcbView>
</views>
</connector>
<connector id="connector33" name="GPIO1" type="male">
<description>GPIO1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector33pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector33pin" terminalId="connector33terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector33pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="GPIO10" type="male">
<description>GPIO10</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="GPIO11" type="male">
<description>GPIO11</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="GPIO12" type="male">
<description>GPIO12</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="GPIO13" type="male">
<description>GPIO13</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector59" name="GPIO14" type="male">
<description>GPIO14</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector59pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector59pin" terminalId="connector59terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector59pad"/>
</pcbView>
</views>
</connector>
<connector id="connector70" name="GPIO15" type="male">
<description>GPIO15</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector70pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector70pin" terminalId="connector70terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector70pad"/>
</pcbView>
</views>
</connector>
<connector id="connector63" name="GPIO16" type="male">
<description>GPIO16</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector63pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector63pin" terminalId="connector63terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector63pad"/>
</pcbView>
</views>
</connector>
<connector id="connector58" name="GPIO17" type="male">
<description>GPIO17</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector58pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector58pin" terminalId="connector58terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector58pad"/>
</pcbView>
</views>
</connector>
<connector id="connector75" name="GPIO18" type="male">
<description>GPIO18</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector75pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector75pin" terminalId="connector75terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector75pad"/>
</pcbView>
</views>
</connector>
<connector id="connector32" name="GPIO2_JDR" type="male">
<description>GPIO2_JDR</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector32pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector32pin" terminalId="connector32terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector32pad"/>
</pcbView>
</views>
</connector>
<connector id="connector54" name="GPIO3_CAM_SCL" type="male">
<description>GPIO3_CAM_SCL</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector54pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector54pin" terminalId="connector54terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector54pad"/>
</pcbView>
</views>
</connector>
<connector id="connector31" name="GPIO4_CAM_SDA" type="male">
<description>GPIO4_CAM_SDA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector31pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector31pin" terminalId="connector31terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector31pad"/>
</pcbView>
</views>
</connector>
<connector id="connector52" name="GPIO5" type="male">
<description>GPIO5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector52pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector52pin" terminalId="connector52terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector52pad"/>
</pcbView>
</views>
</connector>
<connector id="connector53" name="GPIO6" type="male">
<description>GPIO6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector53pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector53pin" terminalId="connector53terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector53pad"/>
</pcbView>
</views>
</connector>
<connector id="connector50" name="GPIO7_BUZZER" type="male">
<description>GPIO7_BUZZER</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector50pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector50pin" terminalId="connector50terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector50pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="GPIO8_CAM_ON" type="male">
<description>GPIO8_CAM_ON</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="GPIO9_CAM_RST" type="male">
<description>GPIO9_CAM_RST</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector82" name="GPS_ANT" type="male">
<description>GPS_ANT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector82pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector82pin" terminalId="connector82terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector82pad"/>
</pcbView>
</views>
</connector>
<connector id="connector14" name="MIC_HF+" type="male">
<description>MIC_HF+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector14pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector14pad"/>
</pcbView>
</views>
</connector>
<connector id="connector15" name="MIC_HF-" type="male">
<description>MIC_HF-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector15pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector15pad"/>
</pcbView>
</views>
</connector>
<connector id="connector12" name="MIC_MT+" type="male">
<description>MIC_MT+</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector13" name="MIN_MT-" type="male">
<description>MIN_MT-</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector13pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector13pad"/>
</pcbView>
</views>
</connector>
<connector id="connector45" name="ON_OFF" type="male">
<description>ON_OFF</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector45pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector45pin" terminalId="connector45terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector45pad"/>
</pcbView>
</views>
</connector>
<connector id="connector74" name="PPS" type="male">
<description>PPS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector74pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector74pin" terminalId="connector74terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector74pad"/>
</pcbView>
</views>
</connector>
<connector id="connector51" name="PWRMON" type="male">
<description>PWRMON</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector51pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector51pin" terminalId="connector51terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector51pad"/>
</pcbView>
</views>
</connector>
<connector id="connector46" name="RESET" type="male">
<description>RESET</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector46pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector46pin" terminalId="connector46terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector46pad"/>
</pcbView>
</views>
</connector>
<connector id="connector72" name="RX_GPS" type="male">
<description>RX_GPS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector72pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector72pin" terminalId="connector72terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector72pad"/>
</pcbView>
</views>
</connector>
<connector id="connector77" name="RX_GPS_BIN" type="male">
<description>RX_GPS_BIN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector77pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector77pin" terminalId="connector77terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector77pad"/>
</pcbView>
</views>
</connector>
<connector id="connector25" name="RX_TRACE" type="male">
<description>RX_TRACE</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector25pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector25pad"/>
</pcbView>
</views>
</connector>
<connector id="connector17" name="SIMCLK" type="male">
<description>SIMCLK</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector17pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector17pad"/>
</pcbView>
</views>
</connector>
<connector id="connector20" name="SIMIN" type="male">
<description>SIMIN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector20pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector20pad"/>
</pcbView>
</views>
</connector>
<connector id="connector19" name="SIMIO" type="male">
<description>SIMIO</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector19pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector19pad"/>
</pcbView>
</views>
</connector>
<connector id="connector18" name="SIMRST" type="male">
<description>SIMRST</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector18pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector18pad"/>
</pcbView>
</views>
</connector>
<connector id="connector21" name="SIMVCC" type="male">
<description>SIMVCC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector21pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector21pad"/>
</pcbView>
</views>
</connector>
<connector id="connector28" name="STAT_LED" type="male">
<description>STAT_LED</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector28pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector28pin" terminalId="connector28terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector28pad"/>
</pcbView>
</views>
</connector>
<connector id="connector67" name="TX_GPS" type="male">
<description>TX_GPS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector67pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector67pin" terminalId="connector67terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector67pad"/>
</pcbView>
</views>
</connector>
<connector id="connector79" name="TX_GPS_BIN" type="male">
<description>TX_GPS_BIN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector79pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector79pin" terminalId="connector79terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector79pad"/>
</pcbView>
</views>
</connector>
<connector id="connector24" name="TX_TRACE" type="male">
<description>TX_TRACE</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector24pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector24pad"/>
</pcbView>
</views>
</connector>
<connector id="connector30" name="VAUX1" type="male">
<description>VAUX1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector30pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector30pin" terminalId="connector30terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector30pad"/>
</pcbView>
</views>
</connector>
<connector id="connector26" name="VBATT" type="male">
<description>VBATT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector26pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector26pad"/>
</pcbView>
</views>
</connector>
<connector id="connector23" name="VRTC" type="male">
<description>VRTC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector23pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector23pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id="GND">
<nodeMember connectorId="connector68"/>
<nodeMember connectorId="connector66"/>
<nodeMember connectorId="connector55"/>
<nodeMember connectorId="connector49"/>
<nodeMember connectorId="connector47"/>
<nodeMember connectorId="connector44"/>
<nodeMember connectorId="connector35"/>
<nodeMember connectorId="connector27"/>
<nodeMember connectorId="connector81"/>
<nodeMember connectorId="connector78"/>
<nodeMember connectorId="connector76"/>
<nodeMember connectorId="connector71"/>
<nodeMember connectorId="connector16"/>
<nodeMember connectorId="connector7"/>
</bus>
</buses>
</module>