<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Boards-WIZ811MJ-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Boards' WIZ811MJ  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>&lt;h3&gt;WIZnet W5100 Network Module with MagJack - WIZ811MJ&lt;/h3&gt;
WIZnet's WIZ811MJ is a breakout board for the W5100 embedded TCP/IP chip. Also included on the board is a RJ-45 MagJack Connector (RJ45 with X'FMR).&lt;br&gt;&lt;br&gt;

See http://www.sparkfun.com/commerce/product_info.php?products_id=9473 for more documentation and info.&lt;br&gt;
&lt;B&gt;**UNPROVEN&lt;/b&gt;</description>
<title>WIZ811MJ</title>
<tags>
<tag>WIZ811MJ</tag>
</tags>
<properties>
<property name="package">wiz811mj</property>
<property name="family">sparkfun wiz811mj</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-boards_wiz811mj_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-boards_wiz811mj_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-boards_wiz811mj_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
<layer layerId="copper0"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/WIZ811MJ.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector26" name="_CS" type="male">
<description>_CS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector26pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector26pad"/>
<p layer="copper1" svgId="connector26pad"/>
</pcbView>
</views>
</connector>
<connector id="connector27" name="_INT" type="male">
<description>_INT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector27pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector27pad"/>
<p layer="copper1" svgId="connector27pad"/>
</pcbView>
</views>
</connector>
<connector id="connector25" name="_RD" type="male">
<description>_RD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector25pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector25pad"/>
<p layer="copper1" svgId="connector25pad"/>
</pcbView>
</views>
</connector>
<connector id="connector21" name="_RESET" type="male">
<description>_RESET</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector21pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector21pad"/>
<p layer="copper1" svgId="connector21pad"/>
</pcbView>
</views>
</connector>
<connector id="connector23" name="_SCS" type="male">
<description>_SCS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector23pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector23pad"/>
<p layer="copper1" svgId="connector23pad"/>
</pcbView>
</views>
</connector>
<connector id="connector24" name="_WR" type="male">
<description>_WR</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector24pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector24pad"/>
<p layer="copper1" svgId="connector24pad"/>
</pcbView>
</views>
</connector>
<connector id="connector30" name="A0" type="male">
<description>A0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector30pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector30pin" terminalId="connector30terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector30pad"/>
<p layer="copper1" svgId="connector30pad"/>
</pcbView>
</views>
</connector>
<connector id="connector31" name="A1" type="male">
<description>A1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector31pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector31pin" terminalId="connector31terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector31pad"/>
<p layer="copper1" svgId="connector31pad"/>
</pcbView>
</views>
</connector>
<connector id="connector14" name="A10" type="male">
<description>A10</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector14pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector14pad"/>
<p layer="copper1" svgId="connector14pad"/>
</pcbView>
</views>
</connector>
<connector id="connector15" name="A11" type="male">
<description>A11</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector15pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector15pad"/>
<p layer="copper1" svgId="connector15pad"/>
</pcbView>
</views>
</connector>
<connector id="connector16" name="A12" type="male">
<description>A12</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector16pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector16pad"/>
<p layer="copper1" svgId="connector16pad"/>
</pcbView>
</views>
</connector>
<connector id="connector17" name="A13" type="male">
<description>A13</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector17pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector17pad"/>
<p layer="copper1" svgId="connector17pad"/>
</pcbView>
</views>
</connector>
<connector id="connector18" name="A14" type="male">
<description>A14</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector18pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector18pad"/>
<p layer="copper1" svgId="connector18pad"/>
</pcbView>
</views>
</connector>
<connector id="connector32" name="A2" type="male">
<description>A2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector32pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector32pin" terminalId="connector32terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector32pad"/>
<p layer="copper1" svgId="connector32pad"/>
</pcbView>
</views>
</connector>
<connector id="connector33" name="A3" type="male">
<description>A3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector33pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector33pin" terminalId="connector33terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector33pad"/>
<p layer="copper1" svgId="connector33pad"/>
</pcbView>
</views>
</connector>
<connector id="connector34" name="A4" type="male">
<description>A4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector34pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector34pin" terminalId="connector34terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector34pad"/>
<p layer="copper1" svgId="connector34pad"/>
</pcbView>
</views>
</connector>
<connector id="connector35" name="A5" type="male">
<description>A5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector35pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector35pin" terminalId="connector35terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector35pad"/>
<p layer="copper1" svgId="connector35pad"/>
</pcbView>
</views>
</connector>
<connector id="connector36" name="A6" type="male">
<description>A6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector36pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector36pin" terminalId="connector36terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector36pad"/>
<p layer="copper1" svgId="connector36pad"/>
</pcbView>
</views>
</connector>
<connector id="connector37" name="A7" type="male">
<description>A7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector37pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector37pin" terminalId="connector37terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector37pad"/>
<p layer="copper1" svgId="connector37pad"/>
</pcbView>
</views>
</connector>
<connector id="connector12" name="A8" type="male">
<description>A8</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector12pad"/>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector13" name="A9" type="male">
<description>A9</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector13pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector13pad"/>
<p layer="copper1" svgId="connector13pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="D0" type="male">
<description>D0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector3pad"/>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="D1" type="male">
<description>D1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector2pad"/>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="D2" type="male">
<description>D2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector5pad"/>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="D3" type="male">
<description>D3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector4pad"/>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="D4" type="male">
<description>D4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector7pad"/>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="D5" type="male">
<description>D5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector6pad"/>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="D6" type="male">
<description>D6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector9pad"/>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="D7" type="male">
<description>D7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector8pad"/>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector10pad"/>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector28" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector28pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector28pin" terminalId="connector28terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector28pad"/>
<p layer="copper1" svgId="connector28pad"/>
</pcbView>
</views>
</connector>
<connector id="connector38" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector38pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector38pin" terminalId="connector38terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector38pad"/>
<p layer="copper1" svgId="connector38pad"/>
</pcbView>
</views>
</connector>
<connector id="connector39" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector39pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector39pin" terminalId="connector39terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector39pad"/>
<p layer="copper1" svgId="connector39pad"/>
</pcbView>
</views>
</connector>
<connector id="connector29" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector29pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector29pin" terminalId="connector29terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector29pad"/>
<p layer="copper1" svgId="connector29pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="MISO" type="male">
<description>MISO</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector1pad"/>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="MOSI" type="male">
<description>MOSI</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector0pad"/>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector22" name="SCLK" type="male">
<description>SCLK</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector22pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector22pad"/>
<p layer="copper1" svgId="connector22pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="VCC" type="male">
<description>VCC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector11pad"/>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
<connector id="connector20" name="VCC" type="male">
<description>VCC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector20pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
</schematicView>
<pcbView>
<p layer="copper0" svgId="connector20pad"/>
<p layer="copper1" svgId="connector20pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id="VCC">
<nodeMember connectorId="connector20"/>
<nodeMember connectorId="connector11"/>
</bus>
<bus id="GND">
<nodeMember connectorId="connector29"/>
<nodeMember connectorId="connector39"/>
<nodeMember connectorId="connector38"/>
<nodeMember connectorId="connector28"/>
<nodeMember connectorId="connector10"/>
</bus>
</buses>
</module>