<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='PowerDriver-Shield-v13'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;strong&gt;Description:&lt;/strong&gt; This shield allows you to use a computer power supply (or other power source) to use your Arduino to switch high current. With RFP30N06LE MOSFETS, you can easily control a lot of current directly from your Arduino.&lt;/p&gt;


&lt;p&gt;


	The board provides 6 PWM outputs via screw terminals. Check the datasheet for the MOSFET below for full specifications on how much current this board can handle.This board is a very easy way to start using MOSFETS for your next high current project.&lt;/p&gt;


&lt;p&gt;


	&lt;strong&gt;Note:&lt;/strong&gt; If you want to stack another shield on top of this one, you will want to double-up on the stackable headers to clear the MOSFETs.&lt;/p&gt;


&lt;p&gt;


	&lt;strong&gt;Documents:&lt;/strong&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/PowerDriver-Shield-v12.pdf&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/PowerDriver-Shield-v12.zip&quot; target=&quot;_blank&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/Components/General/RFP30N06LE.pdf&quot; target=&quot;_blank&quot;&gt;Datasheet&lt;/a&gt; (RFP30N06L)&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Arduino Power Driver Shield</title>
<url>http://www.sparkfun.com/products/10305</url>
<tags>
<tag>Power</tag>
<tag>Driver</tag>
<tag>Mosfet</tag>
</tags>
<properties>
<property name='family'>Power Shield</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/PowerDriver-Shield-v13_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/PowerDriver-Shield-v13_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/PowerDriver-Shield-v13_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/PowerDriver-Shield-v13_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector36' type='male' name='D11-5V'>
<description>D11-5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/><p layer='copper1' svgId='connector36pad'/></pcbView>
</views>
</connector>
<connector id='connector37' type='male' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/><p layer='copper1' svgId='connector37pad'/></pcbView>
</views>
</connector>
<connector id='connector40' type='male' name='D10-5V'>
<description>D10-5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector40pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector40pin' terminalId='connector40terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector40pad'/><p layer='copper1' svgId='connector40pad'/></pcbView>
</views>
</connector>
<connector id='connector41' type='male' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector41pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector41pin' terminalId='connector41terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector41pad'/><p layer='copper1' svgId='connector41pad'/></pcbView>
</views>
</connector>
<connector id='connector42' type='male' name='D9-5V'>
<description>D9-5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad'/><p layer='copper1' svgId='connector42pad'/></pcbView>
</views>
</connector>
<connector id='connector43' type='male' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector43pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector43pin' terminalId='connector43terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector43pad'/><p layer='copper1' svgId='connector43pad'/></pcbView>
</views>
</connector>
<connector id='connector44' type='male' name='D6-12V'>
<description>D6-12V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector44pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector44pin' terminalId='connector44terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector44pad'/><p layer='copper1' svgId='connector44pad'/></pcbView>
</views>
</connector>
<connector id='connector45' type='male' name='12V'>
<description>12V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector45pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector45pin' terminalId='connector45terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector45pad'/><p layer='copper1' svgId='connector45pad'/></pcbView>
</views>
</connector>
<connector id='connector46' type='male' name='D5-12V'>
<description>D5-12V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector46pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector46pin' terminalId='connector46terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector46pad'/><p layer='copper1' svgId='connector46pad'/></pcbView>
</views>
</connector>
<connector id='connector47' type='male' name='12V'>
<description>12V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector47pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector47pin' terminalId='connector47terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector47pad'/><p layer='copper1' svgId='connector47pad'/></pcbView>
</views>
</connector>
<connector id='connector48' type='male' name='D3-12V'>
<description>D3-12V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector48pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector48pin' terminalId='connector48terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector48pad'/><p layer='copper1' svgId='connector48pad'/></pcbView>
</views>
</connector>
<connector id='connector49' type='male' name='12V'>
<description>12V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector49pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector49pin' terminalId='connector49terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector49pad'/><p layer='copper1' svgId='connector49pad'/></pcbView>
</views>
</connector>
<connector id='connector91' type='female' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector91pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector91pin' terminalId='connector91terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector91pad'/><p layer='copper1' svgId='connector91pad'/></pcbView>
</views>
</connector>
<connector id='connector92' type='female' name='5V_ARDUINO'>
<description>5V_ARDUINO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector92pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector92pin' terminalId='connector92terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector92pad'/><p layer='copper1' svgId='connector92pad'/></pcbView>
</views>
</connector>
<connector id='connector93' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector93pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector93pin' terminalId='connector93terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector93pad'/><p layer='copper1' svgId='connector93pad'/></pcbView>
</views>
</connector>
<connector id='connector94' type='female' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector94pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector94pin' terminalId='connector94terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector94pad'/><p layer='copper1' svgId='connector94pad'/></pcbView>
</views>
</connector>
<connector id='connector95' type='female' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector95pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector95pin' terminalId='connector95terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector95pad'/><p layer='copper1' svgId='connector95pad'/></pcbView>
</views>
</connector>
<connector id='connector96' type='female' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector96pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector96pin' terminalId='connector96terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector96pad'/><p layer='copper1' svgId='connector96pad'/></pcbView>
</views>
</connector>
<connector id='connector97' type='female' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector97pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector97pin' terminalId='connector97terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector97pad'/><p layer='copper1' svgId='connector97pad'/></pcbView>
</views>
</connector>
<connector id='connector98' type='female' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector98pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector98pin' terminalId='connector98terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector98pad'/><p layer='copper1' svgId='connector98pad'/></pcbView>
</views>
</connector>
<connector id='connector99' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector99pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector99pin' terminalId='connector99terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector99pad'/><p layer='copper1' svgId='connector99pad'/></pcbView>
</views>
</connector>
<connector id='connector100' type='female' name='D2'>
<description>D2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector100pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector100pin' terminalId='connector100terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector100pad'/><p layer='copper1' svgId='connector100pad'/></pcbView>
</views>
</connector>
<connector id='connector101' type='female' name='D3'>
<description>D3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector101pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector101pin' terminalId='connector101terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector101pad'/><p layer='copper1' svgId='connector101pad'/></pcbView>
</views>
</connector>
<connector id='connector102' type='female' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector102pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector102pin' terminalId='connector102terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector102pad'/><p layer='copper1' svgId='connector102pad'/></pcbView>
</views>
</connector>
<connector id='connector103' type='female' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector103pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector103pin' terminalId='connector103terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector103pad'/><p layer='copper1' svgId='connector103pad'/></pcbView>
</views>
</connector>
<connector id='connector104' type='female' name='D6'>
<description>D6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector104pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector104pin' terminalId='connector104terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector104pad'/><p layer='copper1' svgId='connector104pad'/></pcbView>
</views>
</connector>
<connector id='connector105' type='female' name='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector105pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector105pin' terminalId='connector105terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector105pad'/><p layer='copper1' svgId='connector105pad'/></pcbView>
</views>
</connector>
<connector id='connector106' type='female' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector106pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector106pin' terminalId='connector106terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector106pad'/><p layer='copper1' svgId='connector106pad'/></pcbView>
</views>
</connector>
<connector id='connector107' type='female' name='D9'>
<description>D9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector107pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector107pin' terminalId='connector107terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector107pad'/><p layer='copper1' svgId='connector107pad'/></pcbView>
</views>
</connector>
<connector id='connector108' type='female' name='D10'>
<description>D10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector108pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector108pin' terminalId='connector108terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector108pad'/><p layer='copper1' svgId='connector108pad'/></pcbView>
</views>
</connector>
<connector id='connector109' type='female' name='D11'>
<description>D11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector109pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector109pin' terminalId='connector109terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector109pad'/><p layer='copper1' svgId='connector109pad'/></pcbView>
</views>
</connector>
<connector id='connector110' type='female' name='D12'>
<description>D12</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector110pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector110pin' terminalId='connector110terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector110pad'/><p layer='copper1' svgId='connector110pad'/></pcbView>
</views>
</connector>
<connector id='connector111' type='female' name='D13'>
<description>D13</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector111pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector111pin' terminalId='connector111terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector111pad'/><p layer='copper1' svgId='connector111pad'/></pcbView>
</views>
</connector>
<connector id='connector112' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector112pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector112pin' terminalId='connector112terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector112pad'/><p layer='copper1' svgId='connector112pad'/></pcbView>
</views>
</connector>
<connector id='connector113' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector113pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector113pin' terminalId='connector113terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector113pad'/><p layer='copper1' svgId='connector113pad'/></pcbView>
</views>
</connector>
<connector id='connector114' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector114pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector114pin' terminalId='connector114terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector114pad'/><p layer='copper1' svgId='connector114pad'/></pcbView>
</views>
</connector>
<connector id='connector115' type='female' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector115pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector115pin' terminalId='connector115terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector115pad'/><p layer='copper1' svgId='connector115pad'/></pcbView>
</views>
</connector>
<connector id='connector116' type='female' name='RX'>
<description>RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector116pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector116pin' terminalId='connector116terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector116pad'/><p layer='copper1' svgId='connector116pad'/></pcbView>
</views>
</connector>
<connector id='connector117' type='female' name='TX'>
<description>TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector117pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector117pin' terminalId='connector117terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector117pad'/><p layer='copper1' svgId='connector117pad'/></pcbView>
</views>
</connector>
<connector id='connector118' type='female' name='VIN'>
<description>VIN</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector118pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector118pin' terminalId='connector118terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector118pad'/><p layer='copper1' svgId='connector118pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='5v'>
<nodeMember connectorId='connector37'/>
<nodeMember connectorId='connector41'/>
<nodeMember connectorId='connector43'/>
</bus>
<bus id='12v'>
<nodeMember connectorId='connector45'/>
<nodeMember connectorId='connector47'/>
<nodeMember connectorId='connector49'/>
</bus>
<bus id='gnd'>
<nodeMember connectorId='connector112'/>
<nodeMember connectorId='connector113'/>
<nodeMember connectorId='connector114'/>
</bus>
</buses>
</module>
