<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='Gas_Sensor_Breakout-v12'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Description:&lt;/span&gt; Simple breakout board for the MQ - 3, MQ - 4, MQ - 6 and MQ - 7 gas sensors.&amp;nbsp; All you need is VCC at 5V, GND, and a resistor to an ADC, that is it.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Note: &lt;/span&gt;This is the PCB only. Sensors listed below.&lt;br style=&quot;font-weight: bold;&quot; /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Dimensions:&lt;/span&gt; 16.8mm diameter&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/BreakoutBoards/Gas_Sensor_Breakout-v11.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://wiring.org.co/learning/basics/airqualitymq135.html&quot; target=&quot;_blank&quot;&gt;Wiring Example&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;br /&gt;


	&amp;nbsp;&lt;/p&gt;</description>
<title>Gas Sensor Breakout Board</title>
<url>http://www.sparkfun.com/products/8891</url>
<tags>
<tag>Gas</tag>
</tags>
<properties>
<property name='family'>Gas Breakout</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/Gas_Sensor_Breakout-v12_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/Gas_Sensor_Breakout-v12_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/Gas_Sensor_Breakout-v12_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/Gas_Sensor_Breakout-v12_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector0' type='male' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector0pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector0pin' terminalId='connector0terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector0pad'/><p layer='copper1' svgId='connector0pad'/></pcbView>
</views>
</connector>
<connector id='connector1' type='male' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector1pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector1pin' terminalId='connector1terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector1pad'/><p layer='copper1' svgId='connector1pad'/></pcbView>
</views>
</connector>
<connector id='connector2' type='male' name='B1'>
<description>B1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector2pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector2pin' terminalId='connector2terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector2pad'/><p layer='copper1' svgId='connector2pad'/></pcbView>
</views>
</connector>
<connector id='connector3' type='male' name='B2'>
<description>B2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector3pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector3pin' terminalId='connector3terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector3pad'/><p layer='copper1' svgId='connector3pad'/></pcbView>
</views>
</connector>
<connector id='connector4' type='male' name='H1'>
<description>H1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector4pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector4pin' terminalId='connector4terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector4pad'/><p layer='copper1' svgId='connector4pad'/></pcbView>
</views>
</connector>
<connector id='connector5' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector5pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector5pin' terminalId='connector5terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector5pad'/><p layer='copper1' svgId='connector5pad'/></pcbView>
</views>
</connector>
<connector id='connector6' type='male' name='H1'>
<description>H1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector6pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector6pad'/><p layer='copper1' svgId='connector6pad'/></pcbView>
</views>
</connector>
<connector id='connector7' type='male' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector7pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector7pad'/><p layer='copper1' svgId='connector7pad'/></pcbView>
</views>
</connector>
<connector id='connector8' type='male' name='B1'>
<description>B1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
<connector id='connector9' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='h1'>
<nodeMember connectorId='connector4'/>
<nodeMember connectorId='connector6'/>
</bus>
<bus id='a1'>
<nodeMember connectorId='connector0'/>
<nodeMember connectorId='connector7'/>
</bus>
<bus id='b1'>
<nodeMember connectorId='connector2'/>
<nodeMember connectorId='connector8'/>
</bus>
<bus id='gnd'>
<nodeMember connectorId='connector5'/>
<nodeMember connectorId='connector9'/>
</bus>
</buses>
</module>
