<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='cellular shield-v12'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;strong&gt;D&lt;/strong&gt;&lt;span style=&quot;font-weight: bold;&quot;&gt;escription: &lt;/span&gt;The Cellular Shield for Arduino includes all the parts needed to interface your Arduino with an &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9533&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;SM5100B&lt;/a&gt; cellular module. This allows you to easily add SMS, GSM/GPRS, and TCP/IP functionalities to your Arduino-based project. All you need to add cellular functionality to your Arduino project is a SIM card (pre-paid or straight from your phone) and an antenna and you can start sending Serial.print statements to make calls, send texts and serve web pages!&lt;/p&gt;


&lt;p&gt;


	&amp;nbsp;The main components of the Cellular Shield are a 60-pin &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9535&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;SM5100B connector&lt;/a&gt;, a &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=548&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;SIM card socket&lt;/a&gt;, and an SPX29302 voltage regulator configured to regulate the Arduino&amp;#39;s raw voltage to 3.8V. The board&amp;#39;s red LED indicates power. The Arduino&amp;#39;s reset button is also brought out on the shield.&lt;br /&gt;


	&lt;br /&gt;


	Two solder jumpers on the board allow you to select which serial pins interface with the cellular module - software (D2, D3) or hardware (D0, D1). There is also a 5-pin, 0.1&amp;quot; spaced header with connections for microphone inputs and speaker outputs. Headers are not soldered on, we recommend the &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9280&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;6&lt;/a&gt; and &lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/commerce/product_info.php?products_id=9279&quot; name=&quot;&quot; target=&quot;_self&quot;&gt;8-pin stackable headers&lt;/a&gt;.&lt;br /&gt;


	&lt;br /&gt;


	The SM5100B cellular module &lt;span style=&quot;font-style: italic;&quot;&gt;is&lt;/span&gt; included with this product, however an antenna is not. It is pre-configured to 9600bps.&lt;br /&gt;


	&lt;br /&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;&lt;span style=&quot;font-weight: bold;&quot;&gt;Documents:&lt;/span&gt;&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/DevTools/Arduino/cellular%20shield-v12.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/Code/Cellular_Shield_Passthrough.zip&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Sample Sketch&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/CellularShield/SM5100B%20Datasheet.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;SM5100B Datasheet&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/CellularShield/SM5100B%20AT%20Command%20Set.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;SM5100B AT Command Set&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/CellularShield/SM5100B%20SMS%20App%20Note.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;SM5100B SMS App Note&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/CellularShield/SM5100B%20TCPIP%20App%20Note.pdf&quot; name=&quot;&quot; target=&quot;&quot;&gt;SM5100B TCP/IP App Note&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://tronixstuff.wordpress.com/2011/01/19/tutorial-arduino-and-gsm-cellular-part-one/&quot; target=&quot;_blank&quot;&gt;Arduino Tutorial&lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;</description>
<title>Arduino Cellular Shield</title>
<url>http://www.sparkfun.com/products/9607</url>
<tags>
<tag>Cell</tag>
<tag>Cellular</tag>
<tag>SM5100</tag>
</tags>
<properties>
<property name='family'>Cellular Shield</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/cellular shield-v12_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/cellular shield-v12_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/cellular shield-v12_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/cellular shield-v12_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector9' type='male' name='MIC_N'>
<description>MIC_N</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
<connector id='connector10' type='male' name='MIC_P'>
<description>MIC_P</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad'/><p layer='copper1' svgId='connector10pad'/></pcbView>
</views>
</connector>
<connector id='connector11' type='male' name='SPK_N'>
<description>SPK_N</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad'/><p layer='copper1' svgId='connector11pad'/></pcbView>
</views>
</connector>
<connector id='connector12' type='male' name='SPK_P'>
<description>SPK_P</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
<connector id='connector31' type='female' name='3.3V'>
<description>3.3V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector31pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector31pin' terminalId='connector31terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector31pad'/><p layer='copper1' svgId='connector31pad'/></pcbView>
</views>
</connector>
<connector id='connector32' type='female' name='5V'>
<description>5V</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector32pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector32pin' terminalId='connector32terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector32pad'/><p layer='copper1' svgId='connector32pad'/></pcbView>
</views>
</connector>
<connector id='connector33' type='female' name='A0'>
<description>A0</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector33pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector33pin' terminalId='connector33terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector33pad'/><p layer='copper1' svgId='connector33pad'/></pcbView>
</views>
</connector>
<connector id='connector34' type='female' name='A1'>
<description>A1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector34pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector34pin' terminalId='connector34terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector34pad'/><p layer='copper1' svgId='connector34pad'/></pcbView>
</views>
</connector>
<connector id='connector35' type='female' name='A2'>
<description>A2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector35pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector35pin' terminalId='connector35terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector35pad'/><p layer='copper1' svgId='connector35pad'/></pcbView>
</views>
</connector>
<connector id='connector36' type='female' name='A3'>
<description>A3</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector36pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector36pin' terminalId='connector36terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector36pad'/><p layer='copper1' svgId='connector36pad'/></pcbView>
</views>
</connector>
<connector id='connector37' type='female' name='A4'>
<description>A4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector37pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector37pin' terminalId='connector37terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector37pad'/><p layer='copper1' svgId='connector37pad'/></pcbView>
</views>
</connector>
<connector id='connector38' type='female' name='A5'>
<description>A5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector38pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector38pin' terminalId='connector38terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector38pad'/><p layer='copper1' svgId='connector38pad'/></pcbView>
</views>
</connector>
<connector id='connector39' type='female' name='AREF'>
<description>AREF</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector39pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector39pin' terminalId='connector39terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector39pad'/><p layer='copper1' svgId='connector39pad'/></pcbView>
</views>
</connector>
<connector id='connector40' type='female' name='D-RX'>
<description>D-RX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector40pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector40pin' terminalId='connector40terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector40pad'/><p layer='copper1' svgId='connector40pad'/></pcbView>
</views>
</connector>
<connector id='connector41' type='female' name='D-TX'>
<description>D-TX</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector41pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector41pin' terminalId='connector41terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector41pad'/><p layer='copper1' svgId='connector41pad'/></pcbView>
</views>
</connector>
<connector id='connector42' type='female' name='D4'>
<description>D4</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector42pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector42pin' terminalId='connector42terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector42pad'/><p layer='copper1' svgId='connector42pad'/></pcbView>
</views>
</connector>
<connector id='connector43' type='female' name='D5'>
<description>D5</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector43pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector43pin' terminalId='connector43terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector43pad'/><p layer='copper1' svgId='connector43pad'/></pcbView>
</views>
</connector>
<connector id='connector44' type='female' name='D6'>
<description>D6</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector44pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector44pin' terminalId='connector44terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector44pad'/><p layer='copper1' svgId='connector44pad'/></pcbView>
</views>
</connector>
<connector id='connector45' type='female' name='D7'>
<description>D7</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector45pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector45pin' terminalId='connector45terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector45pad'/><p layer='copper1' svgId='connector45pad'/></pcbView>
</views>
</connector>
<connector id='connector46' type='female' name='D8'>
<description>D8</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector46pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector46pin' terminalId='connector46terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector46pad'/><p layer='copper1' svgId='connector46pad'/></pcbView>
</views>
</connector>
<connector id='connector47' type='female' name='D9'>
<description>D9</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector47pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector47pin' terminalId='connector47terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector47pad'/><p layer='copper1' svgId='connector47pad'/></pcbView>
</views>
</connector>
<connector id='connector48' type='female' name='D10'>
<description>D10</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector48pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector48pin' terminalId='connector48terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector48pad'/><p layer='copper1' svgId='connector48pad'/></pcbView>
</views>
</connector>
<connector id='connector49' type='female' name='D11'>
<description>D11</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector49pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector49pin' terminalId='connector49terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector49pad'/><p layer='copper1' svgId='connector49pad'/></pcbView>
</views>
</connector>
<connector id='connector50' type='female' name='D12'>
<description>D12</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector50pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector50pin' terminalId='connector50terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector50pad'/><p layer='copper1' svgId='connector50pad'/></pcbView>
</views>
</connector>
<connector id='connector51' type='female' name='D13'>
<description>D13</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector51pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector51pin' terminalId='connector51terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector51pad'/><p layer='copper1' svgId='connector51pad'/></pcbView>
</views>
</connector>
<connector id='connector52' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector52pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector52pin' terminalId='connector52terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector52pad'/><p layer='copper1' svgId='connector52pad'/></pcbView>
</views>
</connector>
<connector id='connector53' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector53pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector53pin' terminalId='connector53terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector53pad'/><p layer='copper1' svgId='connector53pad'/></pcbView>
</views>
</connector>
<connector id='connector54' type='female' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector54pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector54pin' terminalId='connector54terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector54pad'/><p layer='copper1' svgId='connector54pad'/></pcbView>
</views>
</connector>
<connector id='connector55' type='female' name='RESET'>
<description>RESET</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector55pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector55pin' terminalId='connector55terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector55pad'/><p layer='copper1' svgId='connector55pad'/></pcbView>
</views>
</connector>
<connector id='connector56' type='female' name='RX-I'>
<description>RX-I</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector56pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector56pin' terminalId='connector56terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector56pad'/><p layer='copper1' svgId='connector56pad'/></pcbView>
</views>
</connector>
<connector id='connector57' type='female' name='TX-O'>
<description>TX-O</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector57pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector57pin' terminalId='connector57terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector57pad'/><p layer='copper1' svgId='connector57pad'/></pcbView>
</views>
</connector>
<connector id='connector58' type='female' name='VRAW'>
<description>VRAW</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector58pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector58pin' terminalId='connector58terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector58pad'/><p layer='copper1' svgId='connector58pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id='gnd'>
<nodeMember connectorId='connector13'/>
<nodeMember connectorId='connector52'/>
<nodeMember connectorId='connector53'/>
<nodeMember connectorId='connector54'/>
</bus>
</buses>
</module>
