<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.15b.02.03.3943" moduleId="GLCD128x64">
    <author>Vince Callahan</author>
    <title>128 x 64 Graphic LCD</title>
    <label>GLCD 128x64</label>
    <date>2010-02-20</date>
    <url>http://www.arduino.cc/playground/Code/GLCDks0108</url>
    <tags/>
    <properties>
        <property name="resolution">128x64</property>
        <property name="family">Display</property>
        <property name="type">GLCD</property>
    </properties>
    <views>
        <iconView>
            <layers image="icon/GLCD_128x64.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/GLCD_128x64.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/GLCD_128x64.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/GLCD_128x64.svg">
                <layer layerId="copper0"/>
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector6" name="7 DB0" type="male">
            <description>Data Input/Output (LSB)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pin"/>
                    <p layer="copper1" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" name="8 DB1" type="male">
            <description>Data Input/Output</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector7pin"/>
                    <p layer="copper1" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" name="9 BD2" type="male">
            <description>Data Input/Output</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector8pin"/>
                    <p layer="copper1" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" name="1 Vss" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                    <p layer="copper1" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" name="10 DB3" type="male">
            <description>Data Input/Output</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector9pin"/>
                    <p layer="copper1" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" name="11 DB4" type="male">
            <description>Data Input/Output</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector10pin"/>
                    <p layer="copper1" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" name="12 DB5" type="male">
            <description>Data Input/Output</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector11pin"/>
                    <p layer="copper1" svgId="connector11pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" name="13 DB6" type="male">
            <description>Data Input/Output</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector12pin"/>
                    <p layer="copper1" svgId="connector12pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" name="14 DB7" type="male">
            <description>Data Input/Output (MSB)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector13pin"/>
                   <p layer="copper1" svgId="connector13pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" name="15 CS1" type="male">
            <description>H: Chip selection for IC 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector14pin"/>
                   <p layer="copper1" svgId="connector14pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector15" name="16 CS2" type="male">
            <description>H: Chip selection for IC 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector15pin"/>
                   <p layer="copper1" svgId="connector15pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector16" name="17 RST" type="male">
            <description>L: Reset</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector16pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector16pin"/>
                    <p layer="copper1" svgId="connector16pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector17" name="18 Vout" type="male">
            <description>Power Supply for LCD Driving</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector17pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector17pin"/>
                    <p layer="copper1" svgId="connector17pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector18" name="19 A(+)" type="male">
            <description>Power Supply for LED Backlight (+)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector18pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector18pin"/>
                    <p layer="copper1" svgId="connector18pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector19" name="20 K(-)" type="male">
            <description>Power Supply for LED Backlight (-)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector19pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector19pin"/>
                   <p layer="copper1" svgId="connector19pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="2 Vdd" type="male">
            <description>+5V Power for logic</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                   <p layer="copper1" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" name="3 Vo" type="male">
            <description>Operating voltage for LCD Driving</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                    <p layer="copper1" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" name="4 D/I" type="male">
            <description>H: Data Input
L: Instruction Code Input</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin"/>
                   <p layer="copper1" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" name="5 R/W" type="male">
            <description>H: Data Read (LCD Module   MPU)
L: Dara Write (LCD Module   MPU)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin"/>
                    <p layer="copper1" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" name="6 Enable" type="male">
            <description>Enable Signal</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pin"/>
                   <p layer="copper1" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>