<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.4.3b.08.08.4406" moduleId="77c36646df552e9fe72f360837f556cc">
    <version replacedby="77c36646df552e9fe72f360837f556ccleg">4</version>
    <author>Lionel Michel</author>
    <title>Battery block 9V</title>
    <label>VCC</label>
    <date>2009-10-23</date>
    <tags>
        <tag>Battery</tag>
        <tag>power supply</tag>
        <tag>user part</tag>
    </tags>
    <properties>
        <property name="family">obsolete Battery</property>
        <property name="voltage" showInLabel="yes">9V</property>
    </properties>
    <description>Your standard 9 Volts battery block</description>
    <views>
        <iconView>
            <layers image="icon/Battery_block_9V82.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <schematicView>
            <layers image="schematic/Battery_block_9V82.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/jumper_2_100mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
        <breadboardView>
            <layers image="breadboard/Battery_block_9V85.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
    </views>
    <connectors>
        <connector id="connector0" name="-" type="male">
            <description>negative side</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" name="+" type="male">
            <description>positive side</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>