<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.1201" moduleId="1001ABDC02">
 <version replacedby="2011BBEC12">1</version>
 <author>Stefan Hermann</author>
 <title>Ceramic Capacitor</title>
 <label>C</label>
 <date>2008-09-23</date>
 <tags>
  <tag>Capacitor</tag>
  <tag>Ceramic Capacitor</tag>
  <tag>fritzing core</tag>
 </tags>
 <properties>
  <property name="family">obsolete Capacitor</property>
  <property name="Capacitance">0.01&#181;F</property>
  <property name="Capacitor Type">Ceramic</property>
  <property name="Rated Voltage">50V</property>
 <property name="package">THT</property></properties>
 <taxonomy>discreteParts.capacitor.ceramic</taxonomy>
 <description>0.01&#181;F Ceramic Disk Capacitor</description>
 <views>
  <iconView>
   <layers image="icon/ceramic_disk_capacitor_ochre_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView fliphorizontal="true" flipvertical="true">
   <layers image="breadboard/ceramic_disk_capacitor_ochre.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/capacitor.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/axial_lay_300mil.svg">
    <layer layerId="copper0"/>
    <layer layerId="silkscreen"/>
   </layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector0" name="pin 0" type="male">
   <description>pin0</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pad"/>
    </pcbView>
   </views>
  </connector>
  <connector id="connector1" name="pin 1" type="male">
   <description>pin1</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pad"/>
    </pcbView>
   </views>
  </connector>
 </connectors>
</module>