<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Sensors-MPR121-QFN20">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Sensors' MPR121 QFN20 -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>MPR121 Capacitive Touch Sensor Controller</description>
<title>MPR121</title>
<tags>
<tag>QFN20</tag>
<tag>MPR121</tag>
<tag>QFN-20-0.4MM</tag>
</tags>
<properties>
<property name="package">qfn-20-0.4mm</property>
<property name="family">sparkfun Touch Sensor</property>
<property name="variant">qfn20</property>
<property name="technology">capacitive</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/QFN-20-0.4MM_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-sensors_mpr121_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-sensors_qfn-20-0.4mm_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/QFN-20-0.4MM_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector3" name="ADDR" type="male">
<description>ADDR</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="ELE0" type="male">
<description>ELE0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="ELE1" type="male">
<description>ELE1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector17" name="ELE10_LED6" type="male">
<description>ELE10_LED6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector17pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector17pad"/>
</pcbView>
</views>
</connector>
<connector id="connector18" name="ELE11_LED7" type="male">
<description>ELE11_LED7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector18pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector18pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="ELE2" type="male">
<description>ELE2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="ELE3" type="male">
<description>ELE3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="ELE4_LED0" type="male">
<description>ELE4_LED0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
<connector id="connector12" name="ELE5_LED1" type="male">
<description>ELE5_LED1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector13" name="ELE6_LED2" type="male">
<description>ELE6_LED2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector13pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector13pad"/>
</pcbView>
</views>
</connector>
<connector id="connector14" name="ELE7_LED3" type="male">
<description>ELE7_LED3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector14pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector14pad"/>
</pcbView>
</views>
</connector>
<connector id="connector15" name="ELE8_LED4" type="male">
<description>ELE8_LED4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector15pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector15pad"/>
</pcbView>
</views>
</connector>
<connector id="connector16" name="ELE9_LED5" type="male">
<description>ELE9_LED5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector16pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector16pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="REXT" type="male">
<description>REXT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="SCL" type="male">
<description>SCL</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="SDA" type="male">
<description>SDA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector19" name="VDD" type="male">
<description>VDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector19pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector19pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="VREG" type="male">
<description>VREG</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="VSS" type="male">
<description>VSS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="~IRQ" type="male">
<description>~IRQ</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>