<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.7.5b.06.14.6067" moduleId="f43b34feed8ba4cccf5782691a06147f">
    <version>4</version>
    <author>www.fritzing.org</author>
    <title>Audio Jack (TRRS) 3.5mm</title>
    <label>TRRS</label>
    <date>2012-05-25</date>
    <tags>
        <tag>audio jack</tag>
        <tag>microphone</tag>
        <tag>sound</tag>
    </tags>
    <properties>
        <property name="family">Audio Connector</property>
        <property name="package">RC-5325A [SMD]</property>
        <property name="channels">TRRS (4 pins)</property>
        <property name="size">3.5 mm</property>
        <property name="part number">LUMBERG JEITA RC-5325A</property>
    </properties>
    <description>Smartphone audio jack with 4 pins (stereo plus microphone), based on the LUMBERG JEITA RC-5325A</description>
    <views>
        <iconView>
            <layers image="breadboard/audio-jack-4pin.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/audio-jack-4pin.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/audio-jack-4pin.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/audio-jack-4pin-3.5mm-smd-lumberg-jeita-rc-5325A.svg">
                <layer layerId="copper1"/>
                <layer layerId="silkscreen"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector3" type="pad" name="RING1" >
            <description>RING 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector3pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="pad" name="RING2" >
            <description>RING 2</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector4pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="pad" name="TIP" >
            <description>TIP</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="pad" name="SLEEVE" >
            <description>SLEEVE</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pad"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="pad" name="TIP" >
            <description>TIP</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pad"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector2pad"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
    
  <buses>
    <bus id="tip">
      <nodeMember connectorId="connector2"/>
      <nodeMember connectorId="connector0"/>
    </bus>
  </buses>
</module>
