<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.5.2b.02.18.4756" moduleId="5613072d61faed3e547f73435c9afc67">
    <version>4</version>
    <author>Dirk van Oosterbosch</author>
    <title>TPA2000D1 Audio Amplifier</title>
    <label>AMP IC</label>
    <date>2009-05-03</date>
    <tags>
        <tag>IC</tag>
        <tag>Audio</tag>
        <tag>Audio Amplifier</tag>
        <tag>Amp</tag>
        <tag>Amplifier</tag>
    </tags>
    <properties>
        <property name="package">DIL16</property>
        <property name="family">Amplifier IC</property>
    </properties>
    <description>2 Watt Filterless Mono Class-D Audio Power Amplifier</description>
    <views>
        <iconView>
            <layers image="icon/TPA2000D1_Audio_Amplifier.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/TPA2000D1_Audio_Amplifier.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/TPA2000D1_AudioAmplifier_schematic.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/dip_16_700mil_pcb.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector15" type="male" name="BYPASS">
            <description>Bypass pin. Connect with 1uF cap to GND</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector15pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector15pin"/>
                    <p layer="copper1" svgId="connector15pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector3" type="male" name="GAIN0">
            <description>Gain Select logic bit 0</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin"/>
                    <p layer="copper1" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector4" type="male" name="GAIN0">
            <description>Gain Select logic bit 1</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin"/>
                    <p layer="copper1" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector5" type="male" name="PVDD">
            <description>Power supply max 5.5V</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pin"/>
                    <p layer="copper1" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector6" type="male" name="OUTP">
            <description>Output Pin (Power)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pin"/>
                    <p layer="copper1" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector7" type="male" name="GND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector7pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector7pin"/>
                    <p layer="copper1" svgId="connector7pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector8" type="male" name="PGND">
            <description>Power ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector8pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector8pin"/>
                    <p layer="copper1" svgId="connector8pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector9" type="male" name="OUTN">
            <description>Output neutral</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector9pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector9pin"/>
                    <p layer="copper1" svgId="connector9pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector10" type="male" name="PVDD1">
            <description>Power Supply max 5.5V</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector10pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector10pin"/>
                    <p layer="copper1" svgId="connector10pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector11" type="male" name="VDD">
            <description>Voltage Supply</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector11pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector11pin"/>
                    <p layer="copper1" svgId="connector11pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector12" type="male" name="ROSC">
            <description>External oscillator Resistor</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector12pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector12pin"/>
                    <p layer="copper1" svgId="connector12pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector0" type="male" name="INP">
            <description>Input Pin (power)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                    <p layer="copper1" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector13" type="male" name="COSC">
            <description>External oscilator Capacitor</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector13pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector13pin"/>
                    <p layer="copper1" svgId="connector13pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="INN">
            <description>Input Pin (neutral)</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                    <p layer="copper1" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector14" type="male" name="AGND">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector14pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector14pin"/>
                    <p layer="copper1" svgId="connector14pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector2" type="male" name="SHUTDOWN">
            <description>Shutdown pin. Low to shutdown</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                    <p layer="copper1" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
