<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.4.1b.07.17.4356" moduleId="33b94ebdb1ef4e7cf0f8425956cfca60">
    <version>4</version>
    <author>tigoe</author>
    <title>Round Pushbutton</title>
    <label>S</label>
    <date>2010-01-19</date>
    <tags>
        <tag>Pushbutton</tag>
        <tag>button</tag>
        <tag>user part</tag>
    </tags>
    <properties>
        <property name="family">Switch - 2 pin</property>
        <property name="switching circuit">SPST</property>
        <property name="default state">Normally Open</property>
    </properties>
    <description>A generic pushbutton.</description>
    <views>
        <iconView>
            <layers image="icon/Pushbuttonc.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/Pushbuttonc.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/pushbutton.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/pushbutton_2_300mil_thick.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector0" type="male" name="leg0">
            <description>leg</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector0pin"/>
                    <p layer="copper0" svgId="connector0pin"/>
                </pcbView>
            </views>
        </connector>
        <connector id="connector1" type="male" name="leg1">
            <description>leg</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper1" svgId="connector1pin"/>
                    <p layer="copper0" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>
    </connectors>
</module>
