<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.6.0b.07.08.5201" moduleId="13f88e58b86d08d73d112f0fb05e6968">
    <version>4</version>
    <author>Alan Smith</author>
    <title>Half breadboard</title>
    <label>Breadboard</label>
    <date>2011-07-09</date>
    <tags>
        <tag>breadboard</tag>
    </tags>
    <properties>
        <property name="size">half+</property>
        <property name="family">Breadboard</property>
    </properties>
    <description>A breadboard for easily prototyping circuits</description>
    <views>
        <breadboardView>
            <layers image="breadboard/Half_breadboard56a.svg">
                <layer layerId="breadboardbreadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="breadboard/Half_breadboard56a.svg">
                <layer layerId="breadboardbreadboard"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="breadboard/Half_breadboard56a.svg">
                <layer layerId="breadboardbreadboard"/>
            </layers>
        </pcbView>
        <iconView>
            <layers image="breadboard/Half_breadboard56a.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
    </views>
    <connectors IgnoreTerminalPoints="true">
      <connector id="pin1A" type="female" name="pin1A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1B" type="female" name="pin1B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1C" type="female" name="pin1C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1D" type="female" name="pin1D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1E" type="female" name="pin1E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1F" type="female" name="pin1F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1G" type="female" name="pin1G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1H" type="female" name="pin1H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1I" type="female" name="pin1I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin1J" type="female" name="pin1J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin1J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin1J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin1J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2A" type="female" name="pin2A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2B" type="female" name="pin2B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2C" type="female" name="pin2C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2D" type="female" name="pin2D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2E" type="female" name="pin2E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2F" type="female" name="pin2F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2G" type="female" name="pin2G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2H" type="female" name="pin2H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2I" type="female" name="pin2I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin2J" type="female" name="pin2J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin2J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin2J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin2J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3A" type="female" name="pin3A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3B" type="female" name="pin3B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3C" type="female" name="pin3C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3D" type="female" name="pin3D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3E" type="female" name="pin3E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3F" type="female" name="pin3F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3G" type="female" name="pin3G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3H" type="female" name="pin3H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3I" type="female" name="pin3I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3J" type="female" name="pin3J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4A" type="female" name="pin4A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4B" type="female" name="pin4B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4C" type="female" name="pin4C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4D" type="female" name="pin4D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4E" type="female" name="pin4E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4F" type="female" name="pin4F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4G" type="female" name="pin4G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4H" type="female" name="pin4H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4I" type="female" name="pin4I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4J" type="female" name="pin4J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5A" type="female" name="pin5A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5B" type="female" name="pin5B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5C" type="female" name="pin5C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5D" type="female" name="pin5D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5E" type="female" name="pin5E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5F" type="female" name="pin5F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5G" type="female" name="pin5G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5H" type="female" name="pin5H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5I" type="female" name="pin5I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5J" type="female" name="pin5J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6A" type="female" name="pin6A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6B" type="female" name="pin6B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6C" type="female" name="pin6C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6D" type="female" name="pin6D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6E" type="female" name="pin6E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6F" type="female" name="pin6F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6G" type="female" name="pin6G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6H" type="female" name="pin6H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6I" type="female" name="pin6I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6J" type="female" name="pin6J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7A" type="female" name="pin7A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7B" type="female" name="pin7B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7C" type="female" name="pin7C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7D" type="female" name="pin7D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7E" type="female" name="pin7E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7F" type="female" name="pin7F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7G" type="female" name="pin7G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7H" type="female" name="pin7H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7I" type="female" name="pin7I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7J" type="female" name="pin7J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8A" type="female" name="pin8A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8B" type="female" name="pin8B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8C" type="female" name="pin8C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8D" type="female" name="pin8D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8E" type="female" name="pin8E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8F" type="female" name="pin8F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8G" type="female" name="pin8G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8H" type="female" name="pin8H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8I" type="female" name="pin8I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin8J" type="female" name="pin8J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin8J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin8J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin8J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9A" type="female" name="pin9A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9B" type="female" name="pin9B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9C" type="female" name="pin9C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9D" type="female" name="pin9D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9E" type="female" name="pin9E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9F" type="female" name="pin9F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9G" type="female" name="pin9G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9H" type="female" name="pin9H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9I" type="female" name="pin9I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9J" type="female" name="pin9J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10A" type="female" name="pin10A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10B" type="female" name="pin10B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10C" type="female" name="pin10C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10D" type="female" name="pin10D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10E" type="female" name="pin10E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10F" type="female" name="pin10F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10G" type="female" name="pin10G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10H" type="female" name="pin10H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10I" type="female" name="pin10I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10J" type="female" name="pin10J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11A" type="female" name="pin11A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11B" type="female" name="pin11B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11C" type="female" name="pin11C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11D" type="female" name="pin11D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11E" type="female" name="pin11E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11F" type="female" name="pin11F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11G" type="female" name="pin11G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11H" type="female" name="pin11H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11I" type="female" name="pin11I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11J" type="female" name="pin11J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12A" type="female" name="pin12A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12B" type="female" name="pin12B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12C" type="female" name="pin12C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12D" type="female" name="pin12D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12E" type="female" name="pin12E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12F" type="female" name="pin12F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12G" type="female" name="pin12G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12H" type="female" name="pin12H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12I" type="female" name="pin12I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12J" type="female" name="pin12J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13A" type="female" name="pin13A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13B" type="female" name="pin13B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13C" type="female" name="pin13C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13D" type="female" name="pin13D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13E" type="female" name="pin13E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13F" type="female" name="pin13F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13G" type="female" name="pin13G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13H" type="female" name="pin13H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13I" type="female" name="pin13I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13J" type="female" name="pin13J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14A" type="female" name="pin14A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14B" type="female" name="pin14B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14C" type="female" name="pin14C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14D" type="female" name="pin14D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14E" type="female" name="pin14E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14F" type="female" name="pin14F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14G" type="female" name="pin14G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14H" type="female" name="pin14H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14I" type="female" name="pin14I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin14J" type="female" name="pin14J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin14J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin14J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin14J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15A" type="female" name="pin15A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15B" type="female" name="pin15B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15C" type="female" name="pin15C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15D" type="female" name="pin15D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15E" type="female" name="pin15E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15F" type="female" name="pin15F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15G" type="female" name="pin15G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15H" type="female" name="pin15H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15I" type="female" name="pin15I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15J" type="female" name="pin15J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16A" type="female" name="pin16A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16B" type="female" name="pin16B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16C" type="female" name="pin16C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16D" type="female" name="pin16D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16E" type="female" name="pin16E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16F" type="female" name="pin16F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16G" type="female" name="pin16G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16H" type="female" name="pin16H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16I" type="female" name="pin16I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16J" type="female" name="pin16J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17A" type="female" name="pin17A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17B" type="female" name="pin17B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17C" type="female" name="pin17C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17D" type="female" name="pin17D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17E" type="female" name="pin17E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17F" type="female" name="pin17F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17G" type="female" name="pin17G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17H" type="female" name="pin17H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17I" type="female" name="pin17I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17J" type="female" name="pin17J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18A" type="female" name="pin18A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18B" type="female" name="pin18B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18C" type="female" name="pin18C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18D" type="female" name="pin18D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18E" type="female" name="pin18E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18F" type="female" name="pin18F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18G" type="female" name="pin18G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18H" type="female" name="pin18H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18I" type="female" name="pin18I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18J" type="female" name="pin18J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19A" type="female" name="pin19A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19B" type="female" name="pin19B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19C" type="female" name="pin19C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19D" type="female" name="pin19D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19E" type="female" name="pin19E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19F" type="female" name="pin19F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19G" type="female" name="pin19G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19H" type="female" name="pin19H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19I" type="female" name="pin19I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19J" type="female" name="pin19J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20A" type="female" name="pin20A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20B" type="female" name="pin20B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20C" type="female" name="pin20C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20D" type="female" name="pin20D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20E" type="female" name="pin20E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20F" type="female" name="pin20F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20G" type="female" name="pin20G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20H" type="female" name="pin20H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20I" type="female" name="pin20I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin20J" type="female" name="pin20J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin20J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin20J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin20J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21A" type="female" name="pin21A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21B" type="female" name="pin21B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21C" type="female" name="pin21C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21D" type="female" name="pin21D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21E" type="female" name="pin21E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21F" type="female" name="pin21F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21G" type="female" name="pin21G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21H" type="female" name="pin21H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21I" type="female" name="pin21I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21J" type="female" name="pin21J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22A" type="female" name="pin22A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22B" type="female" name="pin22B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22C" type="female" name="pin22C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22D" type="female" name="pin22D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22E" type="female" name="pin22E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22F" type="female" name="pin22F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22G" type="female" name="pin22G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22H" type="female" name="pin22H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22I" type="female" name="pin22I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22J" type="female" name="pin22J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23A" type="female" name="pin23A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23B" type="female" name="pin23B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23C" type="female" name="pin23C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23D" type="female" name="pin23D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23E" type="female" name="pin23E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23F" type="female" name="pin23F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23G" type="female" name="pin23G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23H" type="female" name="pin23H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23I" type="female" name="pin23I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23J" type="female" name="pin23J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24A" type="female" name="pin24A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24B" type="female" name="pin24B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24C" type="female" name="pin24C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24D" type="female" name="pin24D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24E" type="female" name="pin24E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24F" type="female" name="pin24F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24G" type="female" name="pin24G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24H" type="female" name="pin24H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24I" type="female" name="pin24I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24J" type="female" name="pin24J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25A" type="female" name="pin25A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25B" type="female" name="pin25B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25C" type="female" name="pin25C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25D" type="female" name="pin25D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25E" type="female" name="pin25E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25F" type="female" name="pin25F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25G" type="female" name="pin25G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25H" type="female" name="pin25H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25I" type="female" name="pin25I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25J" type="female" name="pin25J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26A" type="female" name="pin26A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26B" type="female" name="pin26B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26C" type="female" name="pin26C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26D" type="female" name="pin26D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26E" type="female" name="pin26E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26F" type="female" name="pin26F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26G" type="female" name="pin26G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26H" type="female" name="pin26H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26I" type="female" name="pin26I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin26J" type="female" name="pin26J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin26J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin26J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin26J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27A" type="female" name="pin27A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27B" type="female" name="pin27B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27C" type="female" name="pin27C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27D" type="female" name="pin27D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27E" type="female" name="pin27E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27F" type="female" name="pin27F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27G" type="female" name="pin27G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27H" type="female" name="pin27H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27I" type="female" name="pin27I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27J" type="female" name="pin27J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28A" type="female" name="pin28A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28B" type="female" name="pin28B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28C" type="female" name="pin28C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28D" type="female" name="pin28D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28E" type="female" name="pin28E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28F" type="female" name="pin28F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28G" type="female" name="pin28G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28H" type="female" name="pin28H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28I" type="female" name="pin28I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28J" type="female" name="pin28J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29A" type="female" name="pin29A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29B" type="female" name="pin29B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29C" type="female" name="pin29C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29D" type="female" name="pin29D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29E" type="female" name="pin29E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29F" type="female" name="pin29F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29G" type="female" name="pin29G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29H" type="female" name="pin29H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29I" type="female" name="pin29I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29J" type="female" name="pin29J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30A" type="female" name="pin30A">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30A"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30A"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30A"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30B" type="female" name="pin30B">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30B"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30B"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30B"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30C" type="female" name="pin30C">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30C"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30C"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30C"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30D" type="female" name="pin30D">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30D"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30D"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30D"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30E" type="female" name="pin30E">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30E"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30E"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30E"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30F" type="female" name="pin30F">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30F"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30F"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30F"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30G" type="female" name="pin30G">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30G"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30G"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30G"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30H" type="female" name="pin30H">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30H"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30H"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30H"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30I" type="female" name="pin30I">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30I"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30I"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30I"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30J" type="female" name="pin30J">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30J"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30J"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30J"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3W" type="female" name="pin3W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3X" type="female" name="pin3X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3Y" type="female" name="pin3Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin3Z" type="female" name="pin3Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin3Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin3Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin3Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4W" type="female" name="pin4W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4X" type="female" name="pin4X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4Y" type="female" name="pin4Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin4Z" type="female" name="pin4Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin4Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin4Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin4Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5W" type="female" name="pin5W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5X" type="female" name="pin5X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5Y" type="female" name="pin5Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin5Z" type="female" name="pin5Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin5Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin5Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin5Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6W" type="female" name="pin6W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6X" type="female" name="pin6X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6Y" type="female" name="pin6Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin6Z" type="female" name="pin6Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin6Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin6Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin6Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7W" type="female" name="pin7W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7X" type="female" name="pin7X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7Y" type="female" name="pin7Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin7Z" type="female" name="pin7Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin7Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin7Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin7Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9W" type="female" name="pin9W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9X" type="female" name="pin9X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9Y" type="female" name="pin9Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin9Z" type="female" name="pin9Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin9Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin9Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin9Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10W" type="female" name="pin10W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10X" type="female" name="pin10X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10Y" type="female" name="pin10Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin10Z" type="female" name="pin10Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin10Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin10Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin10Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11W" type="female" name="pin11W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11X" type="female" name="pin11X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11Y" type="female" name="pin11Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin11Z" type="female" name="pin11Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin11Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin11Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin11Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12W" type="female" name="pin12W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12X" type="female" name="pin12X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12Y" type="female" name="pin12Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin12Z" type="female" name="pin12Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin12Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin12Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin12Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13W" type="female" name="pin13W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13X" type="female" name="pin13X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13Y" type="female" name="pin13Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin13Z" type="female" name="pin13Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin13Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin13Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin13Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15W" type="female" name="pin15W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15X" type="female" name="pin15X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15Y" type="female" name="pin15Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin15Z" type="female" name="pin15Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin15Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin15Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin15Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16W" type="female" name="pin16W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16X" type="female" name="pin16X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16Y" type="female" name="pin16Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin16Z" type="female" name="pin16Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin16Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin16Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin16Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17W" type="female" name="pin17W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17X" type="female" name="pin17X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17Y" type="female" name="pin17Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin17Z" type="female" name="pin17Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin17Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin17Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin17Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18W" type="female" name="pin18W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18X" type="female" name="pin18X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18Y" type="female" name="pin18Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin18Z" type="female" name="pin18Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin18Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin18Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin18Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19W" type="female" name="pin19W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19X" type="female" name="pin19X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19Y" type="female" name="pin19Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin19Z" type="female" name="pin19Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin19Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin19Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin19Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21W" type="female" name="pin21W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21X" type="female" name="pin21X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21Y" type="female" name="pin21Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin21Z" type="female" name="pin21Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin21Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin21Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin21Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22W" type="female" name="pin22W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22X" type="female" name="pin22X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22Y" type="female" name="pin22Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin22Z" type="female" name="pin22Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin22Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin22Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin22Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23W" type="female" name="pin23W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23X" type="female" name="pin23X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23Y" type="female" name="pin23Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin23Z" type="female" name="pin23Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin23Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin23Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin23Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24W" type="female" name="pin24W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24X" type="female" name="pin24X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24Y" type="female" name="pin24Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin24Z" type="female" name="pin24Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin24Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin24Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin24Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25W" type="female" name="pin25W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25X" type="female" name="pin25X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25Y" type="female" name="pin25Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin25Z" type="female" name="pin25Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin25Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin25Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin25Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27W" type="female" name="pin27W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27X" type="female" name="pin27X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27Y" type="female" name="pin27Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin27Z" type="female" name="pin27Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin27Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin27Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin27Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28W" type="female" name="pin28W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28X" type="female" name="pin28X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28Y" type="female" name="pin28Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin28Z" type="female" name="pin28Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin28Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin28Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin28Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29W" type="female" name="pin29W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29X" type="female" name="pin29X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29Y" type="female" name="pin29Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin29Z" type="female" name="pin29Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin29Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin29Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin29Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30W" type="female" name="pin30W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30X" type="female" name="pin30X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30Y" type="female" name="pin30Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin30Z" type="female" name="pin30Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin30Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin30Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin30Z"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin31W" type="female" name="pin31W">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin31W"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin31W"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin31W"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin31X" type="female" name="pin31X">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin31X"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin31X"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin31X"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin31Y" type="female" name="pin31Y">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin31Y"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin31Y"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin31Y"/>
        </pcbView>
         </views>
      </connector>
      <connector id="pin31Z" type="female" name="pin31Z">
         <description>breadboard socket</description>
         <views>
           <breadboardView>
             <p layer = "breadboardbreadboard" svgId="pin31Z"/>
           </breadboardView>
           <schematicView>
             <p layer = "breadboardbreadboard" svgId="pin31Z"/>
        </schematicView>
          <pcbView>
             <p layer = "breadboardbreadboard" svgId="pin31Z"/>
        </pcbView>
         </views>
      </connector>    
    </connectors>
    <buses>
      <bus id="bus1-a">
        <nodeMember connectorId="pin1A"/>
           <nodeMember connectorId="pin1B"/>
           <nodeMember connectorId="pin1C"/>
           <nodeMember connectorId="pin1D"/>
           <nodeMember connectorId="pin1E"/>
      </bus>
      <bus id="bus1-f">
           <nodeMember connectorId="pin1F"/>
           <nodeMember connectorId="pin1G"/>
           <nodeMember connectorId="pin1H"/>
           <nodeMember connectorId="pin1I"/>
           <nodeMember connectorId="pin1J"/>     
      </bus>
      <bus id="bus2-a">
        <nodeMember connectorId="pin2A"/>
           <nodeMember connectorId="pin2B"/>
           <nodeMember connectorId="pin2C"/>
           <nodeMember connectorId="pin2D"/>
           <nodeMember connectorId="pin2E"/>
      </bus>
      <bus id="bus2-f">
           <nodeMember connectorId="pin2F"/>
           <nodeMember connectorId="pin2G"/>
           <nodeMember connectorId="pin2H"/>
           <nodeMember connectorId="pin2I"/>
           <nodeMember connectorId="pin2J"/>     
      </bus>
      <bus id="bus3-a">
        <nodeMember connectorId="pin3A"/>
           <nodeMember connectorId="pin3B"/>
           <nodeMember connectorId="pin3C"/>
           <nodeMember connectorId="pin3D"/>
           <nodeMember connectorId="pin3E"/>
      </bus>
      <bus id="bus3-f">
           <nodeMember connectorId="pin3F"/>
           <nodeMember connectorId="pin3G"/>
           <nodeMember connectorId="pin3H"/>
           <nodeMember connectorId="pin3I"/>
           <nodeMember connectorId="pin3J"/>     
      </bus>
      <bus id="bus4-a">
        <nodeMember connectorId="pin4A"/>
           <nodeMember connectorId="pin4B"/>
           <nodeMember connectorId="pin4C"/>
           <nodeMember connectorId="pin4D"/>
           <nodeMember connectorId="pin4E"/>
      </bus>
      <bus id="bus4-f">
           <nodeMember connectorId="pin4F"/>
           <nodeMember connectorId="pin4G"/>
           <nodeMember connectorId="pin4H"/>
           <nodeMember connectorId="pin4I"/>
           <nodeMember connectorId="pin4J"/>     
      </bus>
      <bus id="bus5-a">
        <nodeMember connectorId="pin5A"/>
           <nodeMember connectorId="pin5B"/>
           <nodeMember connectorId="pin5C"/>
           <nodeMember connectorId="pin5D"/>
           <nodeMember connectorId="pin5E"/>
      </bus>
      <bus id="bus5-f">
           <nodeMember connectorId="pin5F"/>
           <nodeMember connectorId="pin5G"/>
           <nodeMember connectorId="pin5H"/>
           <nodeMember connectorId="pin5I"/>
           <nodeMember connectorId="pin5J"/>     
      </bus>
      <bus id="bus6-a">
        <nodeMember connectorId="pin6A"/>
           <nodeMember connectorId="pin6B"/>
           <nodeMember connectorId="pin6C"/>
           <nodeMember connectorId="pin6D"/>
           <nodeMember connectorId="pin6E"/>
      </bus>
      <bus id="bus6-f">
           <nodeMember connectorId="pin6F"/>
           <nodeMember connectorId="pin6G"/>
           <nodeMember connectorId="pin6H"/>
           <nodeMember connectorId="pin6I"/>
           <nodeMember connectorId="pin6J"/>     
      </bus>
      <bus id="bus7-a">
        <nodeMember connectorId="pin7A"/>
           <nodeMember connectorId="pin7B"/>
           <nodeMember connectorId="pin7C"/>
           <nodeMember connectorId="pin7D"/>
           <nodeMember connectorId="pin7E"/>
      </bus>
      <bus id="bus7-f">
           <nodeMember connectorId="pin7F"/>
           <nodeMember connectorId="pin7G"/>
           <nodeMember connectorId="pin7H"/>
           <nodeMember connectorId="pin7I"/>
           <nodeMember connectorId="pin7J"/>     
      </bus>
      <bus id="bus8-a">
        <nodeMember connectorId="pin8A"/>
           <nodeMember connectorId="pin8B"/>
           <nodeMember connectorId="pin8C"/>
           <nodeMember connectorId="pin8D"/>
           <nodeMember connectorId="pin8E"/>
      </bus>
      <bus id="bus8-f">
           <nodeMember connectorId="pin8F"/>
           <nodeMember connectorId="pin8G"/>
           <nodeMember connectorId="pin8H"/>
           <nodeMember connectorId="pin8I"/>
           <nodeMember connectorId="pin8J"/>     
      </bus>
      <bus id="bus9-a">
        <nodeMember connectorId="pin9A"/>
           <nodeMember connectorId="pin9B"/>
           <nodeMember connectorId="pin9C"/>
           <nodeMember connectorId="pin9D"/>
           <nodeMember connectorId="pin9E"/>
      </bus>
      <bus id="bus9-f">
           <nodeMember connectorId="pin9F"/>
           <nodeMember connectorId="pin9G"/>
           <nodeMember connectorId="pin9H"/>
           <nodeMember connectorId="pin9I"/>
           <nodeMember connectorId="pin9J"/>     
      </bus>
      <bus id="bus10-a">
        <nodeMember connectorId="pin10A"/>
           <nodeMember connectorId="pin10B"/>
           <nodeMember connectorId="pin10C"/>
           <nodeMember connectorId="pin10D"/>
           <nodeMember connectorId="pin10E"/>
      </bus>
      <bus id="bus10-f">
           <nodeMember connectorId="pin10F"/>
           <nodeMember connectorId="pin10G"/>
           <nodeMember connectorId="pin10H"/>
           <nodeMember connectorId="pin10I"/>
           <nodeMember connectorId="pin10J"/>     
      </bus>
      <bus id="bus11-a">
        <nodeMember connectorId="pin11A"/>
           <nodeMember connectorId="pin11B"/>
           <nodeMember connectorId="pin11C"/>
           <nodeMember connectorId="pin11D"/>
           <nodeMember connectorId="pin11E"/>
      </bus>
      <bus id="bus11-f">
           <nodeMember connectorId="pin11F"/>
           <nodeMember connectorId="pin11G"/>
           <nodeMember connectorId="pin11H"/>
           <nodeMember connectorId="pin11I"/>
           <nodeMember connectorId="pin11J"/>     
      </bus>
      <bus id="bus12-a">
        <nodeMember connectorId="pin12A"/>
           <nodeMember connectorId="pin12B"/>
           <nodeMember connectorId="pin12C"/>
           <nodeMember connectorId="pin12D"/>
           <nodeMember connectorId="pin12E"/>
      </bus>
      <bus id="bus12-f">
           <nodeMember connectorId="pin12F"/>
           <nodeMember connectorId="pin12G"/>
           <nodeMember connectorId="pin12H"/>
           <nodeMember connectorId="pin12I"/>
           <nodeMember connectorId="pin12J"/>     
      </bus>
      <bus id="bus13-a">
        <nodeMember connectorId="pin13A"/>
           <nodeMember connectorId="pin13B"/>
           <nodeMember connectorId="pin13C"/>
           <nodeMember connectorId="pin13D"/>
           <nodeMember connectorId="pin13E"/>
      </bus>
      <bus id="bus13-f">
           <nodeMember connectorId="pin13F"/>
           <nodeMember connectorId="pin13G"/>
           <nodeMember connectorId="pin13H"/>
           <nodeMember connectorId="pin13I"/>
           <nodeMember connectorId="pin13J"/>     
      </bus>
      <bus id="bus14-a">
        <nodeMember connectorId="pin14A"/>
           <nodeMember connectorId="pin14B"/>
           <nodeMember connectorId="pin14C"/>
           <nodeMember connectorId="pin14D"/>
           <nodeMember connectorId="pin14E"/>
      </bus>
      <bus id="bus14-f">
           <nodeMember connectorId="pin14F"/>
           <nodeMember connectorId="pin14G"/>
           <nodeMember connectorId="pin14H"/>
           <nodeMember connectorId="pin14I"/>
           <nodeMember connectorId="pin14J"/>     
      </bus>
      <bus id="bus15-a">
        <nodeMember connectorId="pin15A"/>
           <nodeMember connectorId="pin15B"/>
           <nodeMember connectorId="pin15C"/>
           <nodeMember connectorId="pin15D"/>
           <nodeMember connectorId="pin15E"/>
      </bus>
      <bus id="bus15-f">
           <nodeMember connectorId="pin15F"/>
           <nodeMember connectorId="pin15G"/>
           <nodeMember connectorId="pin15H"/>
           <nodeMember connectorId="pin15I"/>
           <nodeMember connectorId="pin15J"/>     
      </bus>
      <bus id="bus16-a">
        <nodeMember connectorId="pin16A"/>
           <nodeMember connectorId="pin16B"/>
           <nodeMember connectorId="pin16C"/>
           <nodeMember connectorId="pin16D"/>
           <nodeMember connectorId="pin16E"/>
      </bus>
      <bus id="bus16-f">
           <nodeMember connectorId="pin16F"/>
           <nodeMember connectorId="pin16G"/>
           <nodeMember connectorId="pin16H"/>
           <nodeMember connectorId="pin16I"/>
           <nodeMember connectorId="pin16J"/>     
      </bus>
      <bus id="bus17-a">
        <nodeMember connectorId="pin17A"/>
           <nodeMember connectorId="pin17B"/>
           <nodeMember connectorId="pin17C"/>
           <nodeMember connectorId="pin17D"/>
           <nodeMember connectorId="pin17E"/>
      </bus>
      <bus id="bus17-f">
           <nodeMember connectorId="pin17F"/>
           <nodeMember connectorId="pin17G"/>
           <nodeMember connectorId="pin17H"/>
           <nodeMember connectorId="pin17I"/>
           <nodeMember connectorId="pin17J"/>     
      </bus>
      <bus id="bus18-a">
        <nodeMember connectorId="pin18A"/>
           <nodeMember connectorId="pin18B"/>
           <nodeMember connectorId="pin18C"/>
           <nodeMember connectorId="pin18D"/>
           <nodeMember connectorId="pin18E"/>
      </bus>
      <bus id="bus18-f">
           <nodeMember connectorId="pin18F"/>
           <nodeMember connectorId="pin18G"/>
           <nodeMember connectorId="pin18H"/>
           <nodeMember connectorId="pin18I"/>
           <nodeMember connectorId="pin18J"/>     
      </bus>
      <bus id="bus19-a">
        <nodeMember connectorId="pin19A"/>
           <nodeMember connectorId="pin19B"/>
           <nodeMember connectorId="pin19C"/>
           <nodeMember connectorId="pin19D"/>
           <nodeMember connectorId="pin19E"/>
      </bus>
      <bus id="bus19-f">
           <nodeMember connectorId="pin19F"/>
           <nodeMember connectorId="pin19G"/>
           <nodeMember connectorId="pin19H"/>
           <nodeMember connectorId="pin19I"/>
           <nodeMember connectorId="pin19J"/>     
      </bus>
      <bus id="bus20-a">
        <nodeMember connectorId="pin20A"/>
           <nodeMember connectorId="pin20B"/>
           <nodeMember connectorId="pin20C"/>
           <nodeMember connectorId="pin20D"/>
           <nodeMember connectorId="pin20E"/>
      </bus>
      <bus id="bus20-f">
           <nodeMember connectorId="pin20F"/>
           <nodeMember connectorId="pin20G"/>
           <nodeMember connectorId="pin20H"/>
           <nodeMember connectorId="pin20I"/>
           <nodeMember connectorId="pin20J"/>     
      </bus>
      <bus id="bus21-a">
        <nodeMember connectorId="pin21A"/>
           <nodeMember connectorId="pin21B"/>
           <nodeMember connectorId="pin21C"/>
           <nodeMember connectorId="pin21D"/>
           <nodeMember connectorId="pin21E"/>
      </bus>
      <bus id="bus21-f">
           <nodeMember connectorId="pin21F"/>
           <nodeMember connectorId="pin21G"/>
           <nodeMember connectorId="pin21H"/>
           <nodeMember connectorId="pin21I"/>
           <nodeMember connectorId="pin21J"/>     
      </bus>
      <bus id="bus22-a">
        <nodeMember connectorId="pin22A"/>
           <nodeMember connectorId="pin22B"/>
           <nodeMember connectorId="pin22C"/>
           <nodeMember connectorId="pin22D"/>
           <nodeMember connectorId="pin22E"/>
      </bus>
      <bus id="bus22-f">
           <nodeMember connectorId="pin22F"/>
           <nodeMember connectorId="pin22G"/>
           <nodeMember connectorId="pin22H"/>
           <nodeMember connectorId="pin22I"/>
           <nodeMember connectorId="pin22J"/>     
      </bus>
      <bus id="bus23-a">
        <nodeMember connectorId="pin23A"/>
           <nodeMember connectorId="pin23B"/>
           <nodeMember connectorId="pin23C"/>
           <nodeMember connectorId="pin23D"/>
           <nodeMember connectorId="pin23E"/>
      </bus>
      <bus id="bus23-f">
           <nodeMember connectorId="pin23F"/>
           <nodeMember connectorId="pin23G"/>
           <nodeMember connectorId="pin23H"/>
           <nodeMember connectorId="pin23I"/>
           <nodeMember connectorId="pin23J"/>     
      </bus>
      <bus id="bus24-a">
        <nodeMember connectorId="pin24A"/>
           <nodeMember connectorId="pin24B"/>
           <nodeMember connectorId="pin24C"/>
           <nodeMember connectorId="pin24D"/>
           <nodeMember connectorId="pin24E"/>
      </bus>
      <bus id="bus24-f">
           <nodeMember connectorId="pin24F"/>
           <nodeMember connectorId="pin24G"/>
           <nodeMember connectorId="pin24H"/>
           <nodeMember connectorId="pin24I"/>
           <nodeMember connectorId="pin24J"/>     
      </bus>
      <bus id="bus25-a">
        <nodeMember connectorId="pin25A"/>
           <nodeMember connectorId="pin25B"/>
           <nodeMember connectorId="pin25C"/>
           <nodeMember connectorId="pin25D"/>
           <nodeMember connectorId="pin25E"/>
      </bus>
      <bus id="bus25-f">
           <nodeMember connectorId="pin25F"/>
           <nodeMember connectorId="pin25G"/>
           <nodeMember connectorId="pin25H"/>
           <nodeMember connectorId="pin25I"/>
           <nodeMember connectorId="pin25J"/>     
      </bus>
      <bus id="bus26-a">
        <nodeMember connectorId="pin26A"/>
           <nodeMember connectorId="pin26B"/>
           <nodeMember connectorId="pin26C"/>
           <nodeMember connectorId="pin26D"/>
           <nodeMember connectorId="pin26E"/>
      </bus>
      <bus id="bus26-f">
           <nodeMember connectorId="pin26F"/>
           <nodeMember connectorId="pin26G"/>
           <nodeMember connectorId="pin26H"/>
           <nodeMember connectorId="pin26I"/>
           <nodeMember connectorId="pin26J"/>     
      </bus>
      <bus id="bus27-a">
        <nodeMember connectorId="pin27A"/>
           <nodeMember connectorId="pin27B"/>
           <nodeMember connectorId="pin27C"/>
           <nodeMember connectorId="pin27D"/>
           <nodeMember connectorId="pin27E"/>
      </bus>
      <bus id="bus27-f">
           <nodeMember connectorId="pin27F"/>
           <nodeMember connectorId="pin27G"/>
           <nodeMember connectorId="pin27H"/>
           <nodeMember connectorId="pin27I"/>
           <nodeMember connectorId="pin27J"/>     
      </bus>
      <bus id="bus28-a">
        <nodeMember connectorId="pin28A"/>
           <nodeMember connectorId="pin28B"/>
           <nodeMember connectorId="pin28C"/>
           <nodeMember connectorId="pin28D"/>
           <nodeMember connectorId="pin28E"/>
      </bus>
      <bus id="bus28-f">
           <nodeMember connectorId="pin28F"/>
           <nodeMember connectorId="pin28G"/>
           <nodeMember connectorId="pin28H"/>
           <nodeMember connectorId="pin28I"/>
           <nodeMember connectorId="pin28J"/>     
      </bus>
      <bus id="bus29-a">
        <nodeMember connectorId="pin29A"/>
           <nodeMember connectorId="pin29B"/>
           <nodeMember connectorId="pin29C"/>
           <nodeMember connectorId="pin29D"/>
           <nodeMember connectorId="pin29E"/>
      </bus>
      <bus id="bus29-f">
           <nodeMember connectorId="pin29F"/>
           <nodeMember connectorId="pin29G"/>
           <nodeMember connectorId="pin29H"/>
           <nodeMember connectorId="pin29I"/>
           <nodeMember connectorId="pin29J"/>     
      </bus>
      <bus id="bus30-a">
        <nodeMember connectorId="pin30A"/>
           <nodeMember connectorId="pin30B"/>
           <nodeMember connectorId="pin30C"/>
           <nodeMember connectorId="pin30D"/>
           <nodeMember connectorId="pin30E"/>
      </bus>
      <bus id="bus30-f">
           <nodeMember connectorId="pin30F"/>
           <nodeMember connectorId="pin30G"/>
           <nodeMember connectorId="pin30H"/>
           <nodeMember connectorId="pin30I"/>
           <nodeMember connectorId="pin30J"/>     
      </bus>
      <bus id="bus-W">
        <nodeMember connectorId="pin3W"/>
        <nodeMember connectorId="pin4W"/>
        <nodeMember connectorId="pin5W"/>
        <nodeMember connectorId="pin6W"/>
        <nodeMember connectorId="pin7W"/>    

        <nodeMember connectorId="pin9W"/>
        <nodeMember connectorId="pin10W"/>
        <nodeMember connectorId="pin11W"/>
        <nodeMember connectorId="pin12W"/>
        <nodeMember connectorId="pin13W"/>   
        
        <nodeMember connectorId="pin15W"/>
        <nodeMember connectorId="pin16W"/>
        <nodeMember connectorId="pin17W"/>
        <nodeMember connectorId="pin18W"/>
        <nodeMember connectorId="pin19W"/> 
        
        <nodeMember connectorId="pin21W"/>
        <nodeMember connectorId="pin22W"/>
        <nodeMember connectorId="pin23W"/>
        <nodeMember connectorId="pin24W"/>
        <nodeMember connectorId="pin25W"/>
        
        <nodeMember connectorId="pin27W"/>
        <nodeMember connectorId="pin28W"/>
        <nodeMember connectorId="pin29W"/>
        <nodeMember connectorId="pin30W"/>
        <nodeMember connectorId="pin31W"/>                 
      </bus>
      <bus id="bus-X">
        <nodeMember connectorId="pin3X"/>
           <nodeMember connectorId="pin4X"/>
           <nodeMember connectorId="pin5X"/>
           <nodeMember connectorId="pin6X"/>
           <nodeMember connectorId="pin7X"/>    

           <nodeMember connectorId="pin9X"/>
           <nodeMember connectorId="pin10X"/>
           <nodeMember connectorId="pin11X"/>
           <nodeMember connectorId="pin12X"/>
           <nodeMember connectorId="pin13X"/>   
              
           <nodeMember connectorId="pin15X"/>
           <nodeMember connectorId="pin16X"/>
           <nodeMember connectorId="pin17X"/>
           <nodeMember connectorId="pin18X"/>
           <nodeMember connectorId="pin19X"/> 
              
           <nodeMember connectorId="pin21X"/>
           <nodeMember connectorId="pin22X"/>
           <nodeMember connectorId="pin23X"/>
           <nodeMember connectorId="pin24X"/>
           <nodeMember connectorId="pin25X"/>
              
           <nodeMember connectorId="pin27X"/>
           <nodeMember connectorId="pin28X"/>
           <nodeMember connectorId="pin29X"/>
           <nodeMember connectorId="pin30X"/>
           <nodeMember connectorId="pin31X"/>                 
      </bus>
      <bus id="bus-Y">
        <nodeMember connectorId="pin3Y"/>
           <nodeMember connectorId="pin4Y"/>
           <nodeMember connectorId="pin5Y"/>
           <nodeMember connectorId="pin6Y"/>
           <nodeMember connectorId="pin7Y"/>    

           <nodeMember connectorId="pin9Y"/>
           <nodeMember connectorId="pin10Y"/>
           <nodeMember connectorId="pin11Y"/>
           <nodeMember connectorId="pin12Y"/>
           <nodeMember connectorId="pin13Y"/>   
              
           <nodeMember connectorId="pin15Y"/>
           <nodeMember connectorId="pin16Y"/>
           <nodeMember connectorId="pin17Y"/>
           <nodeMember connectorId="pin18Y"/>
           <nodeMember connectorId="pin19Y"/> 
              
           <nodeMember connectorId="pin21Y"/>
           <nodeMember connectorId="pin22Y"/>
           <nodeMember connectorId="pin23Y"/>
           <nodeMember connectorId="pin24Y"/>
           <nodeMember connectorId="pin25Y"/>
              
           <nodeMember connectorId="pin27Y"/>
           <nodeMember connectorId="pin28Y"/>
           <nodeMember connectorId="pin29Y"/>
           <nodeMember connectorId="pin30Y"/>
           <nodeMember connectorId="pin31Y"/>                 
      </bus>
      <bus id="bus-Z">
        <nodeMember connectorId="pin3Z"/>
           <nodeMember connectorId="pin4Z"/>
           <nodeMember connectorId="pin5Z"/>
           <nodeMember connectorId="pin6Z"/>
           <nodeMember connectorId="pin7Z"/>    

           <nodeMember connectorId="pin9Z"/>
           <nodeMember connectorId="pin10Z"/>
           <nodeMember connectorId="pin11Z"/>
           <nodeMember connectorId="pin12Z"/>
           <nodeMember connectorId="pin13Z"/>   
              
           <nodeMember connectorId="pin15Z"/>
           <nodeMember connectorId="pin16Z"/>
           <nodeMember connectorId="pin17Z"/>
           <nodeMember connectorId="pin18Z"/>
           <nodeMember connectorId="pin19Z"/> 
              
           <nodeMember connectorId="pin21Z"/>
           <nodeMember connectorId="pin22Z"/>
           <nodeMember connectorId="pin23Z"/>
           <nodeMember connectorId="pin24Z"/>
           <nodeMember connectorId="pin25Z"/>
              
           <nodeMember connectorId="pin27Z"/>
           <nodeMember connectorId="pin28Z"/>
           <nodeMember connectorId="pin29Z"/>
           <nodeMember connectorId="pin30Z"/>
           <nodeMember connectorId="pin31Z"/>                 
      </bus>
    </buses>
</module>
