<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-DigitalIC-W5100-">
<!-- generated from Sparkfun Eagle Library 'SparkFun-DigitalIC' W5100  -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>&lt;h3&gt;WIZnet W5100&lt;/h3&gt;
TCP/IP PHY Embedded Chip&lt;br&gt;
See SparkFun catalog # COM-09471&lt;br&gt;
&lt;br&gt;
Package: &lt;b&gt;LQFP-80&lt;/b&gt;,10x10mm,  0.4mm pitch</description>
<title>LQFP-80</title>
<tags>
<tag>LQFP-80</tag>
<tag>W5100</tag>
</tags>
<properties>
<property name="package">lqfp-80</property>
<property name="family">sparkfun Ethernet controller</property>
<property name="chip">W5100</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-digitalic_lqfp-80_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-digitalic_w5100_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-digitalic_lqfp-80_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="breadboard/sparkfun-digitalic_lqfp-80_breadboard.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector54" name="*CS" type="male">
<description>*CS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector54pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector54pin" terminalId="connector54terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector54pad"/>
</pcbView>
</views>
</connector>
<connector id="connector55" name="*INT" type="male">
<description>*INT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector55pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector55pin" terminalId="connector55terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector55pad"/>
</pcbView>
</views>
</connector>
<connector id="connector57" name="*RD" type="male">
<description>*RD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector57pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector57pin" terminalId="connector57terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector57pad"/>
</pcbView>
</views>
</connector>
<connector id="connector58" name="*RESET" type="male">
<description>*RESET</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector58pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector58pin" terminalId="connector58terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector58pad"/>
</pcbView>
</views>
</connector>
<connector id="connector28" name="*SCS" type="male">
<description>*SCS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector28pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector28pin" terminalId="connector28terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector28pad"/>
</pcbView>
</views>
</connector>
<connector id="connector56" name="*WR" type="male">
<description>*WR</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector56pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector56pin" terminalId="connector56terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector56pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="1V8A" type="male">
<description>1V8A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector73" name="1V8A" type="male">
<description>1V8A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector73pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector73pin" terminalId="connector73terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector73pad"/>
</pcbView>
</views>
</connector>
<connector id="connector14" name="1V8D" type="male">
<description>1V8D</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector14pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector14pin" terminalId="connector14terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector14pad"/>
</pcbView>
</views>
</connector>
<connector id="connector15" name="1V8D" type="male">
<description>1V8D</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector15pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector15pin" terminalId="connector15terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector15pad"/>
</pcbView>
</views>
</connector>
<connector id="connector32" name="1V8D" type="male">
<description>1V8D</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector32pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector32pin" terminalId="connector32terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector32pad"/>
</pcbView>
</views>
</connector>
<connector id="connector68" name="1V8D" type="male">
<description>1V8D</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector68pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector68pin" terminalId="connector68terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector68pad"/>
</pcbView>
</views>
</connector>
<connector id="connector10" name="1V8OUT" type="male">
<description>1V8OUT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector10pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector10pin" terminalId="connector10terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector10pad"/>
</pcbView>
</views>
</connector>
<connector id="connector1" name="3V3A" type="male">
<description>3V3A</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector1pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector1pad"/>
</pcbView>
</views>
</connector>
<connector id="connector11" name="3V3D" type="male">
<description>3V3D</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector11pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector11pin" terminalId="connector11terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector11pad"/>
</pcbView>
</views>
</connector>
<connector id="connector17" name="3V3D" type="male">
<description>3V3D</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector17pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector17pin" terminalId="connector17terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector17pad"/>
</pcbView>
</views>
</connector>
<connector id="connector43" name="3V3D" type="male">
<description>3V3D</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector43pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector43pin" terminalId="connector43terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector43pad"/>
</pcbView>
</views>
</connector>
<connector id="connector53" name="ADDR0" type="male">
<description>ADDR0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector53pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector53pin" terminalId="connector53terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector53pad"/>
</pcbView>
</views>
</connector>
<connector id="connector52" name="ADDR1" type="male">
<description>ADDR1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector52pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector52pin" terminalId="connector52terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector52pad"/>
</pcbView>
</views>
</connector>
<connector id="connector41" name="ADDR10" type="male">
<description>ADDR10</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector41pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector41pin" terminalId="connector41terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector41pad"/>
</pcbView>
</views>
</connector>
<connector id="connector40" name="ADDR11" type="male">
<description>ADDR11</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector40pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector40pin" terminalId="connector40terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector40pad"/>
</pcbView>
</views>
</connector>
<connector id="connector39" name="ADDR12" type="male">
<description>ADDR12</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector39pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector39pin" terminalId="connector39terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector39pad"/>
</pcbView>
</views>
</connector>
<connector id="connector38" name="ADDR13" type="male">
<description>ADDR13</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector38pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector38pin" terminalId="connector38terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector38pad"/>
</pcbView>
</views>
</connector>
<connector id="connector37" name="ADDR14" type="male">
<description>ADDR14</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector37pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector37pin" terminalId="connector37terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector37pad"/>
</pcbView>
</views>
</connector>
<connector id="connector51" name="ADDR2" type="male">
<description>ADDR2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector51pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector51pin" terminalId="connector51terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector51pad"/>
</pcbView>
</views>
</connector>
<connector id="connector50" name="ADDR3" type="male">
<description>ADDR3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector50pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector50pin" terminalId="connector50terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector50pad"/>
</pcbView>
</views>
</connector>
<connector id="connector49" name="ADDR4" type="male">
<description>ADDR4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector49pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector49pin" terminalId="connector49terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector49pad"/>
</pcbView>
</views>
</connector>
<connector id="connector48" name="ADDR5" type="male">
<description>ADDR5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector48pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector48pin" terminalId="connector48terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector48pad"/>
</pcbView>
</views>
</connector>
<connector id="connector47" name="ADDR6" type="male">
<description>ADDR6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector47pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector47pin" terminalId="connector47terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector47pad"/>
</pcbView>
</views>
</connector>
<connector id="connector46" name="ADDR7" type="male">
<description>ADDR7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector46pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector46pin" terminalId="connector46terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector46pad"/>
</pcbView>
</views>
</connector>
<connector id="connector45" name="ADDR8" type="male">
<description>ADDR8</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector45pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector45pin" terminalId="connector45terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector45pad"/>
</pcbView>
</views>
</connector>
<connector id="connector44" name="ADDR9" type="male">
<description>ADDR9</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector44pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector44pin" terminalId="connector44terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector44pad"/>
</pcbView>
</views>
</connector>
<connector id="connector70" name="COLLED" type="male">
<description>COLLED</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector70pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector70pin" terminalId="connector70terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector70pad"/>
</pcbView>
</views>
</connector>
<connector id="connector25" name="DATA0" type="male">
<description>DATA0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector25pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector25pin" terminalId="connector25terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector25pad"/>
</pcbView>
</views>
</connector>
<connector id="connector24" name="DATA1" type="male">
<description>DATA1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector24pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector24pin" terminalId="connector24terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector24pad"/>
</pcbView>
</views>
</connector>
<connector id="connector23" name="DATA2" type="male">
<description>DATA2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector23pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector23pin" terminalId="connector23terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector23pad"/>
</pcbView>
</views>
</connector>
<connector id="connector22" name="DATA3" type="male">
<description>DATA3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector22pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector22pin" terminalId="connector22terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector22pad"/>
</pcbView>
</views>
</connector>
<connector id="connector21" name="DATA4" type="male">
<description>DATA4</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector21pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector21pin" terminalId="connector21terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector21pad"/>
</pcbView>
</views>
</connector>
<connector id="connector20" name="DATA5" type="male">
<description>DATA5</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector20pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector20pin" terminalId="connector20terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector20pad"/>
</pcbView>
</views>
</connector>
<connector id="connector19" name="DATA6" type="male">
<description>DATA6</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector19pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector19pin" terminalId="connector19terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector19pad"/>
</pcbView>
</views>
</connector>
<connector id="connector18" name="DATA7" type="male">
<description>DATA7</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector18pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector18pin" terminalId="connector18terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector18pad"/>
</pcbView>
</views>
</connector>
<connector id="connector69" name="FDXLED" type="male">
<description>FDXLED</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector69pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector69pin" terminalId="connector69terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector69pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="GNDA" type="male">
<description>GNDA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector9" name="GNDA" type="male">
<description>GNDA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector76" name="GNDA" type="male">
<description>GNDA</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector76pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector76pin" terminalId="connector76terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector76pad"/>
</pcbView>
</views>
</connector>
<connector id="connector12" name="GNDD" type="male">
<description>GNDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector12pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector12pin" terminalId="connector12terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector12pad"/>
</pcbView>
</views>
</connector>
<connector id="connector13" name="GNDD" type="male">
<description>GNDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector13pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector13pin" terminalId="connector13terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector13pad"/>
</pcbView>
</views>
</connector>
<connector id="connector16" name="GNDD" type="male">
<description>GNDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector16pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector16pin" terminalId="connector16terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector16pad"/>
</pcbView>
</views>
</connector>
<connector id="connector31" name="GNDD" type="male">
<description>GNDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector31pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector31pin" terminalId="connector31terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector31pad"/>
</pcbView>
</views>
</connector>
<connector id="connector42" name="GNDD" type="male">
<description>GNDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector42pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector42pin" terminalId="connector42terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector42pad"/>
</pcbView>
</views>
</connector>
<connector id="connector67" name="GNDD" type="male">
<description>GNDD</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector67pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector67pin" terminalId="connector67terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector67pad"/>
</pcbView>
</views>
</connector>
<connector id="connector65" name="LINKLED" type="male">
<description>LINKLED</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector65pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector65pin" terminalId="connector65terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector65pad"/>
</pcbView>
</views>
</connector>
<connector id="connector26" name="MISO" type="male">
<description>MISO</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector26pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector26pin" terminalId="connector26terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector26pad"/>
</pcbView>
</views>
</connector>
<connector id="connector27" name="MOSI" type="male">
<description>MOSI</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector27pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector27pin" terminalId="connector27terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector27pad"/>
</pcbView>
</views>
</connector>
<connector id="connector2" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector2pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector2pad"/>
</pcbView>
</views>
</connector>
<connector id="connector59" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector59pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector59pin" terminalId="connector59terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector59pad"/>
</pcbView>
</views>
</connector>
<connector id="connector60" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector60pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector60pin" terminalId="connector60terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector60pad"/>
</pcbView>
</views>
</connector>
<connector id="connector61" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector61pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector61pin" terminalId="connector61terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector61pad"/>
</pcbView>
</views>
</connector>
<connector id="connector77" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector77pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector77pin" terminalId="connector77terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector77pad"/>
</pcbView>
</views>
</connector>
<connector id="connector78" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector78pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector78pin" terminalId="connector78terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector78pad"/>
</pcbView>
</views>
</connector>
<connector id="connector79" name="NC" type="male">
<description>NC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector79pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector79pin" terminalId="connector79terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector79pad"/>
</pcbView>
</views>
</connector>
<connector id="connector62" name="OPMODE0" type="male">
<description>OPMODE0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector62pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector62pin" terminalId="connector62terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector62pad"/>
</pcbView>
</views>
</connector>
<connector id="connector63" name="OPMODE1" type="male">
<description>OPMODE1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector63pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector63pin" terminalId="connector63terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector63pad"/>
</pcbView>
</views>
</connector>
<connector id="connector64" name="OPMODE2" type="male">
<description>OPMODE2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector64pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector64pin" terminalId="connector64terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector64pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="RSET_BG" type="male">
<description>RSET_BG</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="RXIN" type="male">
<description>RXIN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="RXIP" type="male">
<description>RXIP</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector71" name="RXLED" type="male">
<description>RXLED</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector71pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector71pin" terminalId="connector71terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector71pad"/>
</pcbView>
</views>
</connector>
<connector id="connector29" name="SCLK" type="male">
<description>SCLK</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector29pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector29pin" terminalId="connector29terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector29pad"/>
</pcbView>
</views>
</connector>
<connector id="connector30" name="SEN" type="male">
<description>SEN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector30pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector30pin" terminalId="connector30terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector30pad"/>
</pcbView>
</views>
</connector>
<connector id="connector66" name="SPDLED" type="male">
<description>SPDLED</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector66pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector66pin" terminalId="connector66terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector66pad"/>
</pcbView>
</views>
</connector>
<connector id="connector36" name="TEST0" type="male">
<description>TEST0</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector36pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector36pin" terminalId="connector36terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector36pad"/>
</pcbView>
</views>
</connector>
<connector id="connector35" name="TEST1" type="male">
<description>TEST1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector35pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector35pin" terminalId="connector35terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector35pad"/>
</pcbView>
</views>
</connector>
<connector id="connector34" name="TEST2" type="male">
<description>TEST2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector34pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector34pin" terminalId="connector34terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector34pad"/>
</pcbView>
</views>
</connector>
<connector id="connector33" name="TEST3" type="male">
<description>TEST3</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector33pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector33pin" terminalId="connector33terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector33pad"/>
</pcbView>
</views>
</connector>
<connector id="connector72" name="TXLED" type="male">
<description>TXLED</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector72pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector72pin" terminalId="connector72terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector72pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="TXON" type="male">
<description>TXON</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="TXOP" type="male">
<description>TXOP</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector74" name="XTLN" type="male">
<description>XTLN</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector74pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector74pin" terminalId="connector74terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector74pad"/>
</pcbView>
</views>
</connector>
<connector id="connector75" name="XTLP" type="male">
<description>XTLP</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector75pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector75pin" terminalId="connector75terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector75pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
<bus id="NC">
<nodeMember connectorId="connector79"/>
<nodeMember connectorId="connector78"/>
<nodeMember connectorId="connector77"/>
<nodeMember connectorId="connector61"/>
<nodeMember connectorId="connector60"/>
<nodeMember connectorId="connector59"/>
<nodeMember connectorId="connector2"/>
</bus>
<bus id="GNDA">
<nodeMember connectorId="connector76"/>
<nodeMember connectorId="connector9"/>
<nodeMember connectorId="connector3"/>
</bus>
<bus id="GNDD">
<nodeMember connectorId="connector67"/>
<nodeMember connectorId="connector42"/>
<nodeMember connectorId="connector31"/>
<nodeMember connectorId="connector16"/>
<nodeMember connectorId="connector13"/>
<nodeMember connectorId="connector12"/>
</bus>
<bus id="3V3D">
<nodeMember connectorId="connector43"/>
<nodeMember connectorId="connector17"/>
<nodeMember connectorId="connector11"/>
</bus>
<bus id="1V8A">
<nodeMember connectorId="connector73"/>
<nodeMember connectorId="connector6"/>
</bus>
<bus id="1V8D">
<nodeMember connectorId="connector68"/>
<nodeMember connectorId="connector32"/>
<nodeMember connectorId="connector15"/>
<nodeMember connectorId="connector14"/>
</bus>
</buses>
</module>