<?xml version='1.0' encoding='UTF-8'?>
<module fritzingVersion='0.5.2b.02.18.4756' moduleId='ADXL345-BreakoutBoard-v13'>
<version>4</version>
<date>2011-07-08</date>
<author>SparkFun</author>
<description>&lt;p&gt;


	&lt;b&gt;Description:&lt;/b&gt; This new version adds 2 standoff holes as well as an extra decoupling capacitor. The ADXL345 is a small, thin, low power, 3-axis accelerometer with high resolution (13-bit) measurement at up to &amp;plusmn;16 g. Digital output data is formatted as 16-bit twos complement and is accessible through either a SPI (3- or 4-wire) or I2C digital interface.&amp;nbsp;&lt;/p&gt;


&lt;p&gt;


	The ADXL345 is well suited to measures the static acceleration of gravity in tilt-sensing applications, as well as dynamic acceleration resulting from motion or shock. Its high resolution (4 mg/LSB) enables measurement of inclination changes less than 1.0&amp;deg;.&lt;/p&gt;


&lt;p&gt;


	Several special sensing functions are provided. Activity and inactivity sensing detect the presence or lack of motion and if the acceleration on any axis exceeds a user-set level. Tap sensing detects single and double taps. Free-fall sensing detects if the device is falling. These functions can be mapped to one of two interrupt output pins. An integrated, patent pending 32-level first in, first out (FIFO) buffer can be used to store data to minimize host processor intervention. Low power modes enable intelligent motion-based power management with threshold sensing and active acceleration measurement at extremely low power dissipation.&lt;/p&gt;


&lt;p&gt;


	&lt;span style=&quot;font-weight: bold;&quot;&gt;Features:&lt;/span&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		2.0-3.6VDC Supply Voltage&lt;/li&gt;


	&lt;li&gt;


		Ultra Low Power: 40uA in measurement mode, 0.1uA in standby@ 2.5V&lt;/li&gt;


	&lt;li&gt;


		Tap/Double Tap Detection&lt;/li&gt;


	&lt;li&gt;


		Free-Fall Detection&lt;/li&gt;


	&lt;li&gt;


		SPI and I2C interfaces&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;b&gt;Documents:&lt;/b&gt;&lt;/p&gt;


&lt;ul&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Sensors/Accelerometer/ADXL345-BreakoutBoard-v13.pdf&quot; target=&quot;_blank&quot;&gt; Schematic&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/datasheets/Sensors/Accelerometer/ADXL345-BreakoutBoard-v13.zip&quot;&gt;Eagle Files&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Sensors/Accelerometer/ADXL345.pdf&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt; Datasheet&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://www.sparkfun.com/tutorials/240&quot; target=&quot;_blank&quot;&gt;Quickstart Guide&lt;/a&gt;&lt;/li&gt;


	&lt;li&gt;


		&lt;a classname=&quot;&quot; href=&quot;http://www.sparkfun.com/datasheets/Sensors/Accelerometer/ADXL345-talktest.zip&quot; name=&quot;&quot; target=&quot;_blank&quot;&gt;Example Code&lt;/a&gt; (ATmega328)&lt;/li&gt;


	&lt;li&gt;


		&lt;a href=&quot;http://bildr.org/2011/03/adxl345-arduino/&quot; target=&quot;_blank&quot;&gt;Bildr Tutorial &lt;/a&gt;&lt;/li&gt;


&lt;/ul&gt;


&lt;p&gt;


	&lt;strong&gt;Replaces: &lt;/strong&gt;&lt;a href=&quot;http://www.sparkfun.com/products/9156&quot; target=&quot;_blank&quot;&gt;SEN-09156&lt;/a&gt;&lt;/p&gt;</description>
<title>Triple Axis Accelerometer Breakout - ADXL345</title>
<url>http://www.sparkfun.com/products/9836</url>
<tags>
<tag>Accelerometer</tag>
<tag>Accel</tag>
</tags>
<properties>
<property name='family'>Accelerometer Breakout</property>
<property name='Range'>+/-2,4,8,16g</property>
<property name='Interface'>Digital</property>
</properties>
<views>
<breadboardView>
<layers image='breadboard/ADXL345-BreakoutBoard-v13_breadboard.svg'>
<layer layerId='breadboard'/>
</layers>
</breadboardView>
<schematicView>
<layers image='schematic/ADXL345-BreakoutBoard-v13_schematic.svg'>
<layer layerId='schematic'/>
</layers>
</schematicView>
<pcbView>
<layers image='pcb/ADXL345-BreakoutBoard-v13_pcb.svg'>
<layer layerId='copper1'/>
<layer layerId='silkscreen'/>
<layer layerId='copper0'/>
</layers>
</pcbView>
<iconView>
<layers image='breadboard/ADXL345-BreakoutBoard-v13_breadboard.svg'>
<layer layerId='icon'/>
</layers>
</iconView>
</views>
<connectors>
<connector id='connector6' type='male' name='GND'>
<description>GND</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector6pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector6pin' terminalId='connector6terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector6pad'/><p layer='copper1' svgId='connector6pad'/></pcbView>
</views>
</connector>
<connector id='connector7' type='male' name='VCC'>
<description>VCC</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector7pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector7pin' terminalId='connector7terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector7pad'/><p layer='copper1' svgId='connector7pad'/></pcbView>
</views>
</connector>
<connector id='connector8' type='male' name='CS'>
<description>CS</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector8pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector8pin' terminalId='connector8terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector8pad'/><p layer='copper1' svgId='connector8pad'/></pcbView>
</views>
</connector>
<connector id='connector9' type='male' name='INT1'>
<description>INT1</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector9pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector9pin' terminalId='connector9terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector9pad'/><p layer='copper1' svgId='connector9pad'/></pcbView>
</views>
</connector>
<connector id='connector10' type='male' name='INT2'>
<description>INT2</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector10pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector10pin' terminalId='connector10terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector10pad'/><p layer='copper1' svgId='connector10pad'/></pcbView>
</views>
</connector>
<connector id='connector11' type='male' name='SDO'>
<description>SDO</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector11pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector11pin' terminalId='connector11terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector11pad'/><p layer='copper1' svgId='connector11pad'/></pcbView>
</views>
</connector>
<connector id='connector12' type='male' name='SDA'>
<description>SDA</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector12pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector12pin' terminalId='connector12terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector12pad'/><p layer='copper1' svgId='connector12pad'/></pcbView>
</views>
</connector>
<connector id='connector13' type='male' name='SCL'>
<description>SCL</description><views>
<breadboardView>
<p layer='breadboard' svgId='connector13pin'/></breadboardView>
<schematicView>
<p layer='schematic' svgId='connector13pin' terminalId='connector13terminal'/></schematicView>
<pcbView>
<p layer='copper0' svgId='connector13pad'/><p layer='copper1' svgId='connector13pad'/></pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>
