<?xml version="1.0" encoding="UTF-8"?>
<module fritzingVersion="0.6.3b.08.16.5401" moduleId="Prolight RGB 3 Watt Star">
    <author>Niclas Hoyer</author>
    <title>Prolight RGB 3 Watt Star</title>
    <label>Power RGB</label>
    <date>2011-07-22</date>
    <tags/>
    <properties>
        <property name="family">LED module</property>
        <property name="type">RGB LED</property>
    </properties>
    <description>PCB mounted RGB LED.</description>
    <views>
        <iconView>
            <layers image="icon/LED_Prolight_RGB.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/LED_Prolight_RGB.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <schematicView>
            <layers image="schematic/LED_Prolight_RGB.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
        <pcbView>
            <layers image="pcb/LED_Prolight_RGB.svg">
                <layer layerId="copper0"/>
                <layer layerId="silkscreen"/>
                <layer layerId="copper1"/>
            </layers>
        </pcbView>
    </views>
    <connectors>
        <connector id="connector1" type="pad" name="B+">
            <description>blue anode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                    <p layer="copper1" svgId="connector1pin"/>
                </pcbView>
            </views>
        </connector>

	<connector id="connector2" type="pad" name="G+">
            <description>green anode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                    <p layer="copper1" svgId="connector2pin"/>
                </pcbView>
            </views>
        </connector>
        
	<connector id="connector3" type="pad" name="R+">
            <description>red anode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector3"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector3pin"/>
                    <p layer="copper1" svgId="connector3pin"/>
                </pcbView>
            </views>
        </connector>
        
	<connector id="connector4" type="pad" name="R-">
            <description>red cathode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector4"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector4pin"/>
                    <p layer="copper1" svgId="connector4pin"/>
                </pcbView>
            </views>
        </connector>
        
	<connector id="connector5" type="pad" name="G-">
            <description>green cathode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector5"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector5pin"/>
                    <p layer="copper1" svgId="connector5pin"/>
                </pcbView>
            </views>
        </connector>
        
	<connector id="connector6" type="pad" name="B-">
            <description>blue cathode</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector6"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector6pin"/>
                    <p layer="copper1" svgId="connector6pin"/>
                </pcbView>
            </views>
        </connector>

    </connectors>
</module>
