<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.1.b.1486" moduleId="1001AAACOptocoupler">
<version>4</version>
 <author>Dirk van Oosterbosch</author>
 <title>Optocoupler</title>
 <label>U</label>
 <date>2008-11-12</date>
 <tags>
  <tag>IC</tag>
  <tag>optocoupler</tag>
  <tag>isolator</tag>
 </tags>
 <properties>
  <property name="family">Optocoupler</property>
 <property name="package">THT</property>
<property name="part">4N35</property>
 </properties>
 <description>Optocoupler - keeps you from frying your stuff!</description>
 <views>
  <iconView>
   <layers image="icon/optocoupler4n35_icon.svg">
    <layer layerId="icon"/>
   </layers>
  </iconView>
  <breadboardView>
   <layers image="breadboard/optocoupler4n35_breadboard.svg">
    <layer layerId="breadboard"/>
   </layers>
  </breadboardView>
  <schematicView>
   <layers image="schematic/optocoupler4n35_schematic.svg">
    <layer layerId="schematic"/>
   </layers>
  </schematicView>
  <pcbView>
   <layers image="pcb/dip_6_300mil_pcb.svg">
    <layer layerId="copper0"/>
    <layer layerId="keepout"/>
    <layer layerId="soldermask"/>
    <layer layerId="silkscreen"/>
    <layer layerId="outline"/>
   <layer layerId="copper1"/></layers>
  </pcbView>
 </views>
 <connectors>
  <connector id="connector3" name="Pin 4" type="male">
   <description>Emitter</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector3pin" terminalId="connector3terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector3pin"/>
    <p layer="copper1" svgId="connector3pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector4" name="Pin 5" type="male">
   <description>Collector</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector4pin" terminalId="connector4terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector4pin"/>
    <p layer="copper1" svgId="connector4pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector5" name="Pin 6" type="male">
   <description>Base</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector5pin" terminalId="connector5terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector5pin"/>
    <p layer="copper1" svgId="connector5pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector0" name="Pin 1" type="male">
   <description>Anode</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector0pin" terminalId="connector0terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector0pin"/>
    <p layer="copper1" svgId="connector0pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector1" name="Pin 2" type="male">
   <description>Cathode</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector1pin" terminalId="connector1terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector1pin"/>
    <p layer="copper1" svgId="connector1pin"/></pcbView>
   </views>
  </connector>
  <connector id="connector2" name="Pin 3" type="male">
   <description>Not Connected</description>
   <views>
    <breadboardView>
     <p layer="breadboard" svgId="connector2pin" terminalId="connector2terminal"/>
    </breadboardView>
    <schematicView>
     <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
    </schematicView>
    <pcbView>
     <p layer="copper0" svgId="connector2pin"/>
    <p layer="copper1" svgId="connector2pin"/></pcbView>
   </views>
  </connector>
 </connectors>
</module>