<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.3.11" moduleId="beab33bd7feee277622ef76dd6e79e4d"><version>4</version>
    <author>Lionel Michel</author>
    <title>Infrared Proximity Sensor</title>
    <label>J</label>
    <date>2009-11-12</date>
    <tags>sensor, input, proximity, distance</tags>
    <properties>
        <property name="family">Distance Sensor</property>
    </properties>
    <views>
        <iconView>
            <layers image="icon/infrared proximity sensor.svg">
                <layer layerId="icon"/>
            </layers>
        </iconView>
        <breadboardView>
            <layers image="breadboard/infrared proximity sensor.svg">
                <layer layerId="breadboard"/>
            </layers>
        </breadboardView>
        <pcbView>
            <layers image="pcb/jumper_3_100mil_pcb.svg">
                <layer layerId="copper0"/>
		<layer layerId="silkscreen"/>
            <layer layerId="copper1"/></layers>
        </pcbView>
        <schematicView>
            <layers image="schematic/infrared proximity sensor.svg">
                <layer layerId="schematic"/>
            </layers>
        </schematicView>
    </views>
    <connectors>
        <connector id="connector0" name="Vout" type="male">
            <description>Output Voltage</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector0pin" legId="connector0leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector0pin"/>
                <p layer="copper1" svgId="connector0pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector1" name="GND" type="male">
            <description>Ground</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector1pin"  legId="connector1leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector1pin" terminalId="connector1terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector1pin"/>
                <p layer="copper1" svgId="connector1pin"/></pcbView>
            </views>
        </connector>
        <connector id="connector2" name="Vcc" type="male">
            <description>Supply Voltage</description>
            <views>
                <breadboardView>
                    <p layer="breadboard" svgId="connector2pin"  legId="connector2leg"/>
                </breadboardView>
                <schematicView>
                    <p layer="schematic" svgId="connector2pin" terminalId="connector2terminal"/>
                </schematicView>
                <pcbView>
                    <p layer="copper0" svgId="connector2pin"/>
                <p layer="copper1" svgId="connector2pin"/></pcbView>
            </views>
        </connector>
    </connectors>
</module>