<?xml version="1.0" encoding="UTF-8"?><module fritzingVersion="0.7.2b" moduleId="SparkFun-Connectors-EB-85A-SMD">
<!-- generated from Sparkfun Eagle Library 'SparkFun-Connectors' EB-85A SMD -->
<version>4</version>
<date>2013-02-13</date>
<label>U</label>
<author>www.fritzing.org</author>
<description>&lt;b&gt;EB-85A Connector&lt;/b&gt;
Proven layout and schematic for ETek 5Hz GPS receiver connector. Spark Fun Electronics SKU : GPS-08297</description>
<title>EB-85A Connector</title>
<tags>
<tag>EB-85A</tag>
<tag>SMD</tag>
</tags>
<properties>
<property name="package">eb-85a</property>
<property name="target">EB-85A</property>
<property name="family">sparkfun GPS Receiver</property>
<property name="variant">smd</property>
</properties>
<views>
<breadboardView>
<layers image="breadboard/sparkfun-connectors_eb-85a_breadboard.svg">
<layer layerId="breadboard"/>
</layers>
</breadboardView>
<schematicView>
<layers image="schematic/sparkfun-connectors_eb-85a_schematic.svg">
<layer layerId="schematic"/>
</layers>
</schematicView>
<pcbView>
<layers image="pcb/sparkfun-connectors_eb-85a_pcb.svg">
<layer layerId="copper1"/>
<layer layerId="silkscreen"/>
</layers>
</pcbView>
<iconView>
<layers image="icon/EB-85A.svg">
<layer layerId="icon"/>
</layers>
</iconView>
</views>
<connectors>
<connector id="connector9" name="BATT" type="male">
<description>BATT</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector9pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector9pin" terminalId="connector9terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector9pad"/>
</pcbView>
</views>
</connector>
<connector id="connector3" name="GND" type="male">
<description>GND</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector3pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector3pin" terminalId="connector3terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector3pad"/>
</pcbView>
</views>
</connector>
<connector id="connector8" name="PPS" type="male">
<description>PPS</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector8pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector8pin" terminalId="connector8terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector8pad"/>
</pcbView>
</views>
</connector>
<connector id="connector5" name="RX1" type="male">
<description>RX1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector5pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector5pin" terminalId="connector5terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector5pad"/>
</pcbView>
</views>
</connector>
<connector id="connector7" name="RX2" type="male">
<description>RX2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector7pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector7pin" terminalId="connector7terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector7pad"/>
</pcbView>
</views>
</connector>
<connector id="connector4" name="TX1" type="male">
<description>TX1</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector4pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector4pin" terminalId="connector4terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector4pad"/>
</pcbView>
</views>
</connector>
<connector id="connector6" name="TX2" type="male">
<description>TX2</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector6pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector6pin" terminalId="connector6terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector6pad"/>
</pcbView>
</views>
</connector>
<connector id="connector0" name="VCC" type="male">
<description>VCC</description>
<views>
<breadboardView>
<p layer="breadboard" svgId="connector0pin"/>
</breadboardView>
<schematicView>
<p layer="schematic" svgId="connector0pin" terminalId="connector0terminal"/>
</schematicView>
<pcbView>
<p layer="copper1" svgId="connector0pad"/>
</pcbView>
</views>
</connector>
</connectors>
<buses>
</buses>
</module>